{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-N9"]
[]
[]
[]
[]
["","","","","","3AMXM52N2V1B9"]
["Уровень звуковой мощности","Отопление","","","дБA","59"]
["","Охлаждение","","","дБA","59"]
["Размеры","Блок","","Высота","мм","734"]
["","","","Ширина","мм","974"]
["","","","Глубина","мм","401"]
["Масса","Блок","","","кг","57"]
["Двигатель вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","420"]
["","","Нагревание","Самый низкий","об/мин","420"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-10"]
["","","","Макс.","°C сух.т.","46"]
["Уровень звукового давления","Охлаждение","","Ном.","дБA","46"]
["","Hагрев","","Ном.","дБA","47"]
["Хладагент","Тип","","","","R-32"]
["","Заправка","","","кг","1.8"]
["","Заправка","","","tCO2Eq","1.22"]
["","ПГП","","","","675"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","25 (1)"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 30 м)"]
["","перепад уровня","IU - OU","Макс.","м","15"]
["","","IU - IU","Макс.","м","7.5"]
["Подсоединение труб","Общая длина трубопроводов","Система","Фактическая","м","50"]
["Стандартные аксессуары","Installation manual","","","","1"]
["","Drain cap","","","","3"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Электропитание","Фаза","","","","1~"]
["","Частота","","","Гц","50"]
["","Напряжение","","","V","220-240"]
["Примечания","","","","","(1) - Для одного помещения"]
["","","","","","(2) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","(3) - Электрические параметры см. в отдельных чертежах"]
["","","","","","(4) - Содержит фторированные парниковые газы"]