{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-A"]
[]
[]
[]
[]
["","","","","","3MXM40A2V1B","3MXM52A2V1B","3MXM68A2V1B"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","734","734","734"]
["","","","Ширина","мм","974","974","974"]
["","","","Глубина","мм","408","408","408"]
["Масса","Блок","","","кг","57","57","62"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-10","-10","-10"]
["","","","Макс.","°C сух.т.","46","46","46"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБA","46","46","48"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБA","47","47","48"]
["Хладагент","Тип","","","","R-32","R-32","R-32"]
["","Заправка","","","кг","1.8","1.8","2"]
["","Заправка","","","tCO2Eq","1.22","1.22","1.35"]
["","ПГП","","","","675","675","675"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","25 (1)","25","25 (1)"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 30 м)","0,02 (для длины труб свыше 30 м)","0,02 (для длины труб свыше 30 м)"]
["","перепад уровня","IU - OU","Макс.","м","15","15","15"]
["","","IU - IU","Макс.","м","7.5","7.5","7.5"]
["Подсоединение труб","Общая длина трубопроводов","Система","Фактическая","м","50 (2)","50","50"]
["Стандартные аксессуары","Installation manual","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["","Reducer assembly","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Электропитание","Фаза","","","","1~","1~","1~"]
["","Частота","","","Гц","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240"]
["Примечания","","","","","(1) - Для одного помещения","(1) - Для одного помещения"]
["","","","","","(2) - Для комбинации с CVXM-A, FVXM-A — максимальная длина трубопровода 30 м.","(2) - Для комбинации с CVXM-A, FVXM-A — максимальная длина трубопровода 30 м."]
["","","","","","","","(1) - Для одного помещения"]