{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N8"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B8","3MXM52N2V1B8"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","734","734"]
["","","","Ширина","мм","974","974"]
["","","","Глубина","мм","401","401"]
["Масса","Блок","","","kg","57","57"]
["Двигатель вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","420","420"]
["","","Нагревание","Самый низкий","об/мин","420","420"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°CDB","-10","-10"]
["","","","Макс.","°CDB","46","46"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБ(A)","46","46"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБ(A)","47.0","47.0"]
["Хладагент","Тип","","","","R-32","R-32"]
["","Заправка","","","kg","1.8","1.8"]
["","Заправка","","","tCO2Eq","1.22","1.22"]
["","ПГП","","","","675.0","675.0"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","25","25"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 30 м)","0,02 (для длины труб свыше 30 м)"]
["","перепад уровня","IU - OU","Макс.","м","15.0","15.0"]
["","","IU - IU","Макс.","м","7.5","7.5"]
["Подсоединение труб","Общая длина трубопроводов","Система","Фактическая","м","50","50"]
["Стандартные аксессуары","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Электропитание","Фаза","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Напряжение","","","В","220-240","220-240"]
["Примечания","","","","","(1) - Для одного помещения","(1) - Для одного помещения"]
["","","","","","(2) - Для комбинации с CVXM-A, FVXM-A — максимальная длина трубопровода 30 м.","(2) - Для комбинации с CVXM-A, FVXM-A — максимальная длина трубопровода 30 м."]