{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":8,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXS-E"]
[]
[]
[]
[]
["","","","","","4MXS80E3V3B","4MXS80E3V3B2","4MXS80E7V3B"]
["Размеры","Блок","","Высота","мм","770","770"]
["","","","Ширина","мм","900","900"]
["","","","Глубина","мм","320","320"]
["Масса","Блок","","","кг","72","72"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-10","-10"]
["","","","Макс.","°C сух.т.","46","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-15","-15"]
["","","","Макс.","°CWB","18","18"]
["Уровень звукового давления","Охлаждение","","Ном.","дБ(A)","48","48"]
["","Hагрев","","Ном.","дБ(A)","49","49"]
["Хладагент","Тип","","","","R-410A","R-410A"]
["","Заправка","","","кг","2.99","2.99"]
["","ПГП","","","","2,087.5","2,087.5"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 30 м)","0,02 (для длины труб свыше 30 м)"]
["","Перепад уровней","IU - OU","Макс.","м","15","15"]
["","","IU - IU","Макс.","м","7.5","7.5"]
["","Общая длина трубопроводов","Система","Фактическая","м","70","70"]
["Стандартные аксессуары","Инструкции по установке","","","","1","1"]
["","Сливная пробка","","","","1","1"]
["","Узел переходника","","","","1","1"]
["Power supply","Фаза","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Напряжение","","","V","230","230"]
["Примечания","","","","","(1) - Охлаждение: темп. внутри помещения: 27°CDB, 19,0°CWB; темп. наружного воздуха 35°CDB; длина эквивалентного трубопровода: 7,5 м","(1) - Охлаждение: темп. внутри помещения: 27°CDB, 19,0°CWB; темп. наружного воздуха 35°CDB; длина эквивалентного трубопровода: 7,5 м"]
["","","","","","(2) - Нагрев: темп. в помещении: 20°CDB; темп. наружного воздуха 7°CDB, 6°CWB; эквивалентная длина труб с хладагентом: 7,5 м","(2) - Нагрев: темп. в помещении: 20°CDB; темп. наружного воздуха 7°CDB, 6°CWB; эквивалентная длина труб с хладагентом: 7,5 м"]
["","","","","","(3) - Содержит фторированные парниковые газы","(3) - Содержит фторированные парниковые газы"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","","","770"]
["","","","Ширина","мм","","","900"]
["","","","Глубина","мм","","","320"]
["Масса","Блок","","","кг","","","72"]
["Компрессор","Тип","","","","","","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","","","-10"]
["","","","Макс.","°C сух.т.","","","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","","","-15"]
["","","","Макс.","°CWB","","","15.5"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБ(A)","","","48"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБ(A)","","","49"]
["Хладагент","Тип","","","","","","R-410A"]
["","Заправка","","","кг","","","2.99"]
["","Заправка","","","tCO2Eq","","","6.2"]
["","ПГП","","","","","","2087.5"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","","","25"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","","","0,02 (для длины труб свыше 30 м)"]
["","перепад уровня","IU - OU","Макс.","м","","","15"]
["","","IU - IU","Макс.","м","","","7.5"]
["Подсоединение труб","Общая длина трубопроводов","Система","Фактическая","м","","","70"]
["Стандартные аксессуары","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["Электропитание","Фаза","","","","","","1~"]
["","Частота","","","Гц","","","50"]
["","Напряжение","","","V","","","230"]