{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MWXM-A9"]
[]
[]
[]
[]
["","","","","","5MWXM68A2V1B9","5MWXM90A2V1B9"]
["Размеры","Блок","","Высота","мм","734","734"]
["","","","Ширина","мм","1,040","1,040"]
["","","","Глубина","мм","408","408"]
["Масса","Блок","","","кг","69","73"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-10","-10"]
["","","","Макс.","°C сух.т.","46","46"]
["Уровень звукового давления","Охлаждение","","Ном.","дБA","48","52"]
["","Hагрев","","Ном.","дБA","49","53"]
["Хладагент","Тип","","","","R-32","R-32"]
["","Заправка","","","кг","2","2.4"]
["","Заправка","","","tCO2Eq","1.35","1.62"]
["","ПГП","","","","675","675"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","25 (2)","25 (3)"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 30 м)","0,02 (для длины труб свыше 30 м)"]
["","перепад уровня","IU - OU","Макс.","м","15 (3)","15"]
["","","IU - IU","Макс.","м","7.5 (3)","7.5 (3)"]
["Подсоединение труб","Общая длина трубопроводов","Система","Фактическая","м","60","75"]
["Стандартные аксессуары","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","2","2"]
["Электропитание","Фаза","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Напряжение","","","V","220-440","220-240"]
["Примечания","","","","","(1) - Рабочий диапазон см. в отдельных чертежах","(1) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","(2) - Для одного помещения","(2) - Для одного помещения"]
["","","","","","(3) - Для одного помещения (данные о комбинации с FBA71/100/125 и EKHWET и CKHWS см. в руководстве по установке)","(3) - Для одного помещения (данные о комбинации с FBA71/100/125 и EKHWET и CKHWS см. в руководстве по установке)"]
["","","","","","(4) - Содержит фторированные парниковые газы","(4) - Содержит фторированные парниковые газы"]