{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5XXM-A"]
[]
[]
[]
[]
["","","","","","5XXM68A2V1B","5XXM90A2V1B"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","734","734"]
["","","","Ширина","мм","1040","1040"]
["","","","Глубина","мм","408","408"]
["Масса","Блок","","","кг","69.0","73.0"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-10","-10"]
["","","","Макс.","°C сух.т.","50","50"]
["Уровень звукового давления","Охлаждение","","Ном.","дБA","48.0 (2)","52.0 (2)"]
["","Hагрев","","Ном.","дБA","49.0 (2), 51.0 (3)","53.0 (2), 55.0 (3)"]
["Хладагент","Тип","","","","R-32","R-32"]
["","Заправка","","","кг","2.00","2.40"]
["","Хладагент-=-Заправка-=-Экв. т CO2","","","Экв. т CO2","1.35","1.62"]
["","ПГП","","","","675","675.0"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","25 (4) (5)","25 (5) (4)"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 30 м)","0,02 (для длины труб свыше 30 м)"]
["","перепад уровня","IU - OU","Макс.","м","15.0 (5)","15.0 (5)"]
["","","IU - IU","Макс.","м","7.5 (5)","7.5 (5)"]
["Подсоединение труб","Общая длина трубопроводов","Система","Фактическая","м","60","75"]
["Стандартные аксессуары","Инструкции по установке","","","","1","1"]
["","Сливная крышка","","","","3","3"]
["","Сливная пробка","","","","1","1"]
["","Узел переходника","","","","1","1"]
["","Пакет для винтов","","","","2","2"]
["Диапазон энергоэффективности","","","","","A+++ ~ D","A+++ ~ D"]
["Электропитание","Фаза","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Электропитание-=-Напряжение-=-В","","","В","220-240","220-240"]
["Примечания","","","","","(1) - Рабочий диапазон см. на отдельных чертежах","(1) - Рабочий диапазон см. на отдельных чертежах"]
["","","","","","(2) - For DX combination","(2) - For DX combination"]
["","","","","","(3) - For Space heating operation of CHVX07 unit","(3) - For Space heating operation of CHVX07 unit"]
["","","","","","(4) - Для одного помещения","(4) - Для одного помещения"]
["","","","","","(5) - For combination with FBA71/100/125 refer to installation manual","(5) - For combination with FBA71/100/125 refer to installation manual"]
["","","","","","(6) - Содержит фторированные парниковые газы","(6) - Содержит фторированные парниковые газы"]