{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-C / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ACQ71CV1 / AZQS71B2V1B","ACQ100CV1 / AZQS100B8V1B","ACQ125CV1 / AZQS125B8V1B"]
["Холодопроизводительность","Ном.","","kW","6.8","9.5","12.1"]
["Space cooling","SEER","","","4.65","4.65"]
["","Годовое потребление энергии","","кВтч/г","512","716"]
["","Производительность","Pрасч.","kW","6.80","9.50"]
["","Класс энергоэффективности","","","B","B"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","kW","6.33","7.60"]
["","SCOP/A","","","3.80","3.80"]
["","Класс энергоэффективности","","","A","A"]
["","Годовое потребление энергии","","кВтч/г","2,332","2,800"]
["Номинальная эффективность","Annual energy consumption","","кВтч","1,025","1,480","2,010"]
["","EER","","","3.31","3.21","3.01"]
["","COP","","","3.61","3.61","3.41"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","B","A"]
["","","Нагрев","","A","A"]
["Теплопроизводительность","Ном.","","kW","7.50","10.80","13.5"]
["Примечания","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]