{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Уровень звукового давления","Hагрев","","Выс.","дБA","","44","","47"]
["","","","Ном.","дБA","","41","","44"]
["","","","Тихая работа","дБA","","36","","41"]
["","","","Низк.","дБA","","38","","43"]
["","Охлаждение","","Тихая работа","дБA","","36","","41"]
["","","","Низк.","дБA","","38","","43"]
["","","","Выс.","дБA","","44","","47"]
["","","","Ном.","дБA","","41","","44"]
["Стандартные аксессуары","Инструкции по установке","","","","","Инструкции по установке","","Инструкции по установке"]
["","Руководство по эксплуатации","","","","","Руководство по эксплуатации","","Руководство по эксплуатации"]
["","Винты","","","","","Винты","","Винты"]
["","Шайба","","","","","Шайба","","Шайба"]
["","Беспроводной пульт дистанционного управления","","","","","Беспроводной пульт дистанционного управления","","Беспроводной пульт дистанционного управления"]
["","Крышка-решетка с фиксатором","","","","","Крышка-решетка с фиксатором","","Крышка-решетка с фиксатором"]
["","Батарея","","","","","Батарея","","Батарея"]
["Системы управления","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Подсоединения труб","Liquid","","OD","мм","","9.52","","9.52"]
["","Газ","","НД","мм","","15.88","","15.88"]
["","Drain","","","","","19.05","","19.05"]
["Входная мощность","Охлаждение","","Ном.","кВт","","0.094","","0.137"]
["","Hагрев","","Ном.","кВт","","0.094","","0.137"]
["Уровень звуковой мощности","Охлаждение","","","дБA","","56","","60"]
["","Отопление","","","дБA","","56","","60"]
["Размеры","Блок","","Ширина","мм","","820","","820"]
["","","","Глубина","мм","","820","","820"]
["","","","Высота","мм","","300","","300"]
["Корпус","Материал","","","","","Оцинкованная сталь","","Оцинкованная сталь"]
["Вес","Блок","","","кг","","39","","39"]
["Вентилятор","Расход воздуха","Hагрев","Выс.","м³/мин","","29.2","","34.0"]
["","","","Низк.","м³/мин","","21.0","","26.3"]
["","","","Ном.","м³/мин","","24.4","","29.2"]
["","","Охлаждение","Низк.","м³/мин","","21.0","","26.3"]
["","","","Ном.","м³/мин","","24.4","","29.2"]
["","","","Выс.","м³/мин","","29.2","","34.0"]
["","","","Тихая работа","м³/мин","","17.6","","22.1"]
["","","Охлаждение","Тихая работа","м³/мин","","17.6","","22.1"]
["Декоративная панель","Вес","","","кг","","4","","4"]
["","Размеры","","Высота","мм","","82","","82"]
["","","","Глубина","мм","","990","","990"]
["","","","Ширина","мм","","990","","990"]
["","Цвет","","","","","Белый","","Белый"]
["Power supply","Phase","","","","","1~","","1~"]
["","Наименование","","","","","V1","","V1"]
["","Частота","","","Гц","","50","","50"]
["","Напряжение","","","V","","220-240","","220-240"]
["Вентилятор","Расход воздуха","Hагрев","Тихая работа","м³/мин","15","","22.1"]
["Входная мощность","Hагрев","","Ном.","кВт","0.067","","0.137"]
["","Охлаждение","","Ном.","кВт","0.067","","0.137"]
["Вентилятор","Расход воздуха","Охлаждение","Тихая работа","м³/мин","15","","22.1"]
["Корпус","Материал","","","","Оцинкованная сталь","","Оцинкованная сталь"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","265","","300"]
["","","","Ширина","мм","820","","820"]
["","","","Глубина","мм","820","","820"]
["Масса","Блок","","","кг","31","","39"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","24.4","","34"]
["","","","Ном.","м³/мин","20.5","","29.2"]
["","","","Низк.","м³/мин","17.6","","26.3"]
["","","Hагрев","Выс.","м³/мин","24.4","","34"]
["","","","Ном.","м³/мин","20.5","","29.2"]
["","","","Низк.","м³/мин","17.6","","26.3"]
["Уровень звуковой мощности","Охлаждение","","","дБA","54","","60"]
["","Отопление","","","дБA","54","","60"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","41","","47"]
["","","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБA","38","","44"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","35","","43"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБA","32","","41"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","41","","47"]
["","","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБA","38","","44"]
["","","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","35","","43"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБA","32","","41"]
["Подсоединение труб","Жидкость","","НД","мм","9.52","","9.52"]
["","Газ","","НД","мм","15.88","","15.88"]
["","Дренаж","","","","19.05","","19.05"]
["Декоративна панель","Размеры","","Высота","мм","82","","82"]
["","","","Ширина","мм","990","","990"]
["","","","Глубина","мм","990","","990"]
["","Масса","","","кг","4","","4"]
["Системы управления","Инфракрасный пульт ДУ","","","","ARCWLA","","ARCWLA"]
["","Проводной пульт дистанционного управления","","","","ARCWB","","ARCWB"]
["Стандартные аксессуары","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Электропитание","Фаза","","","","1~","","1~"]
["","Частота","","","Гц","50","","50"]
["","Напряжение","","","V","220-240","","220-240"]