{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":9,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C"]
[]
[]
[]
[]
["","","","","","AHQ71CV1","AHQ100CV1","AHQ125CV1","AHQ140CV1"]
["Входная мощность","Hагрев","","Ном.","кВт","0.106","0.149"]
["","Охлаждение","","Ном.","кВт","0.106","0.149"]
["Вентилятор","Внешнее статическое давление","","Выс.","Па","0","0","0","0"]
["","","","Низк.","Па","0","0","0","0"]
["Холодопроизводительность","Общая производительность","","Ном.","кВт","","","12.10","13.00"]
["Теплопроизводительность","Общая производительность","","Ном.","кВт","","","13.5","15.5"]
["Корпус","Цвет","","","","Белый","Белый","Белый","Белый"]
["","Материал","","","","Оцинкованная сталь","Оцинкованная сталь"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","260","260","260","285"]
["","","","Ширина","мм","1320","1538","1790","1900"]
["","","","Глубина","мм","634","634","634","680"]
["Масса","Блок","","","kg","38","45","65","70"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","23.8","31.1","34.4","43.9"]
["","","","Ном.","м³/мин","21.3","27.8","31","39"]
["","","","Средн.","м³/мин","","","31","39"]
["","","","Низк.","м³/мин","18.9","24.8","27.2","28.3"]
["","","Hагрев","Выс.","м³/мин","23.8","31.1","34.4","43.9"]
["","","","Ном.","м³/мин","21.3","27.8","30.6","39.1"]
["","","Нагрев","Средн.","м³/мин","","","30.6","39.1"]
["","","Hагрев","Низк.","м³/мин","18.9","24.8","27.2","28.3"]
["","Внешнее статическое давление","","Ном.","Па","0","0","0","0"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","59","64","65","71"]
["","Отопление","","","дБ(A)","62","64","65","71"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","49","52","52","56"]
["","","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБ(A)","48","47"]
["","","","Средн.","дБ(A)","","","50","53"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","46","46","49","46"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","49","52","52","56"]
["","Нагрев","","Средн.","дБ(A)","","","50","53"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБ(A)","48","47"]
["","","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","46","46","49","46"]
["Подсоединение труб","Жидкость","","НД","мм","9.52","9.52","9.52","9.52"]
["","Газ","","НД","мм","15.88","15.88","15.9","15.9"]
["","Дренаж","","","","19.05","19.05"]
["Системы управления","Инфракрасный пульт ДУ","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","Проводной пульт дистанционного управления","","","","ARCWB","ARCWB"]
["Стандартные аксессуары","Installation manual","","","","Installation manual","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control"]
["","Battery","","","","Battery","Battery"]
["","Сливная труба","","","","Drain pipe","Drain pipe"]
["","Screw for wireless remote","","","","Screw for wireless remote","Screw for wireless remote"]
["","Ferrite Core","","","","Ferrite Core","Ferrite Core"]
["","Installation manual (Ferrite Core)","","","","Installation manual (Ferrite Core)","Installation manual (Ferrite Core)"]
["","Outdoor wiring diagram","","","","Outdoor wiring diagram","Outdoor wiring diagram"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","Drain hose","","","","Drain hose","Drain hose"]
["Электропитание","Фаза","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Напряжение","","","В","220-240","220-240"]