{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B","CTXM15R5V1B"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.029","0.029"]
["","Hагрев","","Ном.","кВт","0.023","0.023"]
["Корпус","Цвет","","","","Белый","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","295","295"]
["","","","Ширина","мм","778","778"]
["","","","Глубина","мм","272","272"]
["Масса","Блок","","","кг","10","10"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","10.5","10.5"]
["","","","Средн.","м³/мин","7.5","7.5"]
["","","","Низк.","м³/мин","5.7","5.7"]
["","","","Тихая работа","м³/мин","4.3","4.3"]
["","","Hагрев","Выс.","м³/мин","9.3","9.3"]
["","","Нагрев","Средн.","м³/мин","8.2","8.2"]
["","","Hагрев","Низк.","м³/мин","6.2","6.2"]
["","","","Тихая работа","м³/мин","5.1","5.1"]
["Уровень звуковой мощности","Охлаждение","","","дБA","57","57"]
["","Отопление","","","дБA","54","54"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","41","41"]
["","","","Средн.","дБA","33","33"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","25","25"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБA","19","19"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","39","39"]
["","Нагрев","","Средн.","дБA","34","34"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","26","26"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБA","20","20"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35"]
["","Газ","","НД","мм","9.5","9.5"]
["","Дренаж","","","","18","18"]
["Системы управления","Infrared remote control","","","","ARC466A67","ARC466A67"]
["Системы управления","Проводной пульт дистанционного управления","","","","BRC073A1","BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","WLAN adapter kit","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Электропитание","Наименование","","","","V1","V1"]
["","Фаза","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Напряжение","","","V","220-240","220-240"]