{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCM010A51"]
[]
[]
[]
[]
["","","","","DCM010A51."]
["Connectable unit","","","","Внутренний, наружный, гидроблок, типы вентиляции для точек управления iTM"]
["Вход","ПК","Программное обеспечение","","Microsoft Windows 7, 8, 8.1, 10, Microsoft Server 2012 и 2016"]
["Максимальное количество подсоединяемых внутренних блоков","","","","2,500 (2)"]
["Максимальное количество подсоединяемых наружных блоков","","","","400 (3)"]
["Примечания","","","","(1) - Совместимо с версиями Oracle PMS: Opera v5.0.03.03 e43, v5.0.04.01 e24, v5.0.04.02 e17, v5.0.04.02 e17, v5.0.04.03 e10, v5.0.05.00 и более поздних версий"]
["","","","","(2) - 5 x 500 внутренних блоков на контроллер iTM"]
["","","","","(3) - 5 x 80 наружных систем на контроллер iTM"]
["","","","","(4) - Бесплатное для скачивания программное обеспечение, лицензионный ключ в физическом формате (распечатка)"]
["","","","","(5) - Требуется 1 лицензионный DCM010A51 и DCM007A51 для каждого контроллера iTM"]