{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSX-D"]
[]
[]
[]
[]
["","","","","","EBSX11P30DG","EBSX11P50DG","EBSX16P30DG","EBSX16P50DG","EBSX11P30DF (Archived)","EBSX11P50DF (Archived)","EBSX16P30DF (Archived)","EBSX16P50DF (Archived)"]
["Корпус","Цвет","","","","Транспортный белый (RAL9016) / Транспортный черный (RAL9017)","Транспортный белый (RAL9016) / Транспортный черный (RAL9017)","Транспортный белый (RAL9016) / Транспортный черный (RAL9017)","Транспортный белый (RAL9016) / Транспортный черный (RAL9017)","Транспортный белый (RAL9016) / Транспортный черный (RAL9017)","Транспортный белый (RAL9016) / Транспортный черный (RAL9017)","Транспортный белый (RAL9016) / Транспортный черный (RAL9017)","Транспортный белый (RAL9016) / Транспортный черный (RAL9017)"]
["","Материал","","","","Ударостойкий полипропилен","Ударостойкий полипропилен","Ударостойкий полипропилен","Ударостойкий полипропилен","Ударостойкий полипропилен","Ударостойкий полипропилен","Ударостойкий полипропилен","Ударостойкий полипропилен"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","1893","1910","1893","1910","1893","1910","1893","1910"]
["","","","Ширина","мм","594","792","594","792","594","792","594","792"]
["","","","Глубина","мм","680","817","680","817","680","817","680","817"]
["Масса","Блок","","","кг","93","114","93","114","93","114","93","114"]
["PED","Категория","","","","Категория II","Категория II","Категория II","Категория II","Категория II","Категория II","Категория II","Категория II"]
["Хладагент","Тип","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","ПГП","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["","Заправка","","","кг","3.80","3.80","3.80","3.80","3.80","3.80","3.80","3.80"]
["","Хладагент-=-Заправка-=-Экв. т CO2","","","Экв. т CO2","2.57","2.57","2.57","2.57","2.57","2.57","2.57","2.57"]
["Уровень звуковой мощности","Уровень звуковой мощности-=-Ном.-=-дБA","","","дБA","44.7","44.7","49.0","49.0","44.7","44.7","49.0","49.0"]
["Уровень звукового давления","Ном.","","","дБA","36.8","36.8","40.3","40.3","36.8","36.8","40.3","40.3"]
["Рабочий диапазон","Hагрев","Сторона воды","Мин.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Макс.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","Сторона воды","Мин.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Макс.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["Электропитание","Фаза","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50","50","50","50","50"]
["","Электропитание-=-Напряжение-=-В","","","В","230","230","230","230","230","230","230","230"]
["Примечания","","","","","(1) - Теплопотери согласно EN12897","(1) - Теплопотери согласно EN12897","(1) - Теплопотери согласно EN12897","(1) - Теплопотери согласно EN12897","(1) - Теплопотери согласно EN12897","(1) - Теплопотери согласно EN12897","(1) - Теплопотери согласно EN12897","(1) - Теплопотери согласно EN12897"]
["","","","","","(2) - См. чертеж с указанием пределов рабочих характеристик","(2) - См. чертеж с указанием пределов рабочих характеристик","(2) - См. чертеж с указанием пределов рабочих характеристик","(2) - См. чертеж с указанием пределов рабочих характеристик","(2) - См. чертеж с указанием пределов рабочих характеристик","(2) - См. чертеж с указанием пределов рабочих характеристик","(2) - См. чертеж с указанием пределов рабочих характеристик","(2) - См. чертеж с указанием пределов рабочих характеристик"]