{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBX-E6V / ERGA-EVH"]
[]
[]
[]
[]
["","","","","","EHBX08EF6V / ERGA06EAV3H","EHBX08EA6V / ERGA06EAV3H"]
["Теплопроизводительность","Ном.","","","кВт","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)"]
["Холодопроизводительность","Ном.","","","кВт","5.96 (1), 5.09 (2)","5.96 (1), 5.09 (2)"]
["Входная мощность","Hагрев","","Ном.","кВт","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)"]
["","Охлаждение","","Ном.","кВт","1.06 (1), 1.55 (2)","1.06 (1), 1.55 (2)"]
["COP","","","","","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)"]
["EER","","","","","5.61 (1), 3.28 (2)","5.61 (1), 3.28 (2)"]
["Отопление","Среднеклимат. темп. воды на выходе 55°C","Общ.","SCOP","","3.28","3.28"]
["","","","Класс сезонной эффективности отопления помещений","","A++","A++"]
["","Среднеклимат. темп. воды на выходе 35°C","Общ.","SCOP","","4.52","4.52"]
["","","","Класс сезонной эффективности отопления помещений","","A+++","A+++"]
["Диапазон энергоэффективности","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Примечания","","","","","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]