{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EV"]
[]
[]
[]
[]
["","","","","","ERGA04EAV3"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","740"]
["","","","Ширина","мм","884"]
["","","","Глубина","мм","388"]
["Масса","Блок","","","кг","58.5"]
["Рабочий диапазон","Охлаждение","","Рабочий диапазон-=-Охлаждение-=-Мин.-=-°CDB","°C сух.т.","10"]
["","","","Рабочий диапазон-=-Охлаждение-=-Макс.-=-°CDB","°C сух.т.","43"]
["","Бытовая горячая вода","","Мин.","°C сух.т.","-25"]
["","ГВС","","Рабочий диапазон-=-ГВС-=-Макс.-=-°CDB","°C сух.т.","35"]
["Уровень звуковой мощности","Hагрев","","Ном.","дБA","58 (1)"]
["","Охлаждение","","Ном.","дБA","61 (1)"]
["Уровень звукового давления","Hагрев","","Ном.","дБA","44 (1)"]
["","Охлаждение","","Ном.","дБA","48 (1)"]
["Хладагент","Тип","","","","R-32"]
["","ПГП","","","","675.0"]
["","Хладагент-=-Заправка-=-Экв. т CO2","","","Экв. т CO2","1.01"]
["","Заправка","","","кг","1.50"]
["Подсоединение труб","Жидкость","","НД","мм","6"]
["","Газ","","НД","мм","15.9"]
["Подсоединения труб","Дренаж","","НД","мм","18"]
["","перепад уровня","IU - OU","Макс.","м","20.0"]
["Подсоединение труб","Теплоизоляция","","","","Трубопроводы для жидкости и газа"]
["Электропитание","Наименование","","","","V3"]
["","Фаза","","","","1N~"]
["","Частота","","","Гц","50"]
["","Электропитание-=-Напряжение-=-В","","","В","230"]
["Ток","Рекомендуемые предохранители","","","A","20"]
["Примечания","","","","","(1) - Охлаждение Ta 35°C - LWE 18°C ( DT = 5°C ); Нагрев Ta DB/WB 7°C/6°C - LWC 35°C ( DT = 5°C )"]