{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERLA-DV37"]
[]
[]
[]
[]
["","","","","","ERLA16D2V37","ERLA16DAV37"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","870","870"]
["","","","Ширина","мм","1100","1100"]
["","","","Глубина","мм","460","460"]
["Масса","Блок","","","кг","101","101"]
["Вентилятор","Расход воздуха","Hагрев","Выс.","м³/мин","85.0","85.0"]
["","","Охлаждение","Выс.","м³/мин","85","85"]
["Рабочий диапазон","Охлаждение","","Рабочий диапазон-=-Охлаждение-=-Мин.-=-°CDB","°C сух.т.","10","10"]
["","","","Рабочий диапазон-=-Охлаждение-=-Макс.-=-°CDB","°C сух.т.","43","43"]
["","Бытовая горячая вода","","Мин.","°C сух.т.","-25","-25"]
["","ГВС","","Рабочий диапазон-=-ГВС-=-Макс.-=-°CDB","°C сух.т.","25 (1), 35 (1)","25 (1), 35 (1)"]
["Уровень звуковой мощности","Hагрев","","Ном.","дБA","62.0 (2)","62.0 (2)"]
["Уровень звукового давления","Hагрев","","Ном.","дБA","48.0 (2)","48.0 (2)"]
["Хладагент","Тип","","","","R-32","R-32"]
["","ПГП","","","","675.0","675.0"]
["","Хладагент-=-Заправка-=-Экв. т CO2","","","Экв. т CO2","2.57","2.57"]
["","Заправка","","","кг","3.8","3.8"]
["Подсоединение труб","Жидкость","","НД","мм","9.5","9.5"]
["","Газ","","НД","мм","15.9","15.9"]
["Подсоединения труб","Дренаж","","НД","мм","26","26"]
["","перепад уровня","IU - OU","Макс.","м","30.0","30.0"]
["Подсоединение труб","Теплоизоляция","","","","Трубопроводы для жидкости и газа","Трубопроводы для жидкости и газа"]
["Электропитание","Наименование","","","","V3","V3"]
["","Фаза","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Электропитание-=-Напряжение-=-В","","","В","230","230"]
["Ток","Рекомендуемые предохранители","","","A","32","32"]
["Примечания","","","","","(1) - Более подробная информация приведена на чертеже рабочего диапазона","(1) - Более подробная информация приведена на чертеже рабочего диапазона"]
["","","","","","(2) - Измеряется при перепаде давления 10 кПа в системе нагрева, температуре воды на выходе 47–55°С и температуре в помещении 20°С. 7°C/6°С (сух.т./вл.т.)","(2) - Измеряется при перепаде давления 10 кПа в системе нагрева, температуре воды на выходе 47–55°С и температуре в помещении 20°С. 7°C/6°С (сух.т./вл.т.)"]