{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":9,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWYT-CZI"]
[]
[]
[]
[]
["","","","","","EWYT021CZI-A1","EWYT032CZI-A1","EWYT040CZI-A1","EWYT064CZI-A2"]
["Корпус","Цвет","","","","Слоновая кость","Слоновая кость","Слоновая кость","Слоновая кость"]
["","Материал","","","","Оцинкованный и покрашенный стальной лист","Оцинкованный и покрашенный стальной лист","Оцинкованный и покрашенный стальной лист","Оцинкованный и покрашенный стальной лист"]
["Размеры","Блок","","Высота","мм","700","700","700","700"]
["","","","Ширина","мм","1,120","1,120","1,120","1,120"]
["","","","Глубина","мм","830","830","830","830"]
["Масса","Блок","","","кг","133","144","144","172"]
["Уровень звуковой мощности","Ном.","","","дБA","63.0","64.5","64.5","66.0"]
["Рабочий диапазон","Hагрев","Сторона воды","Мин.","°C","20","20","20","20"]
["","","","Макс.","°C","60","60","60","60"]
["","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-20","-20","-20","-20"]
["","","Сторона воды","Мин.","°C","4","4","4","4"]
["","","","Макс.","°C","20","20","20","20"]
["Электропитание","Фаза","","","","3N~","3N~","3N~","3N~"]
["","Частота","","","Гц","50","50","50","50"]
["","Напряжение","","","В","400","400","400","400"]