{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Корпус","Цвет","","","","Белый","Белый"]
["","Материал","","","","Полимер","Полимер"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","290","340"]
["","","","Ширина","мм","1050","1200"]
["","","","Глубина","мм","269","262"]
["Масса","Блок","","","kg","14","18"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","16.2","23"]
["","","","Средн.","м³/мин","13.4","21.1"]
["","","","Низк.","м³/мин","12.1","18.7"]
["","","Hагрев","Выс.","м³/мин","16.9","23"]
["","","Нагрев","Средн.","м³/мин","14.2","20.9"]
["","","Hагрев","Низк.","м³/мин","12.7","18.7"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","61","65"]
["","Отопление","","","дБ(A)","61","65"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","45","49"]
["","","","Средн.","дБ(A)","42","45"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","40","41"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","45","49"]
["","Нагрев","","Средн.","дБ(A)","42","45"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","40","41"]
["Подсоединение труб","Жидкость","","НД","мм","9.52","9.52"]
["","Газ","","НД","мм","15.9","15.9"]
["","Дренаж","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Электропитание","Фаза","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Напряжение","","","В","220-240","220-240"]
["Стандартные аксессуары","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Примечания","","","","","(1) - Номинальные значения холодопроизводительности основаны на: темп. внутри помещения: 27°C с.т., 19°С вл.т., температура наружного воздуха: 35°C c.т., эквивалентная длина трубы с хладагентом: 5 м, перепад высот: 0 м."]
["","","","","","(2) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м."]
["Стандартные аксессуары","Screw cover","","","","","3"]