{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":12,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9)"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB9","FBA50A2VEB9","FBA60A2VEB9","FBA71A2VEB9","FBA100A2VEB","FBA125A2VEB","FBA140A2VEB"]
["Холодопроизводительность","Общая производительность","","Ном.","кВт","","","","","","14.00","15.40"]
["Теплопроизводительность","Общая производительность","","Ном.","кВт","","","","","","13.5","15.5"]
["Корпус","Цвет","","","","Не покрашен (оцинкован)","Не покрашен (оцинкован)","Не покрашен (оцинкован)","Не покрашен (оцинкован)","Не покрашен (оцинкован)","Не покрашен (оцинкован)","Не покрашен (оцинкован)"]
["","Материал","","","","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали"]
["Размеры","Блок","","Высота","мм","245","245","245","245","245","245","245"]
["","","","Ширина","мм","700","700","1000","1000","1400","1400","1400"]
["","","","Глубина","мм","800","800","800","800","800","800","800"]
["Масса","Блок","","","кг","28.0","28.0","35.0","35.0","46.0","46.0","46.0"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","15.0","15.0","18.0","18.0","29.0","34.0","34.0"]
["","","","Средн.","м³/мин","12.5","12.5","15.0","15.0","24.5","29.0","29.0"]
["","","","Низк.","м³/мин","10.5","10.5","12.5","12.5","20.0","23.5","23.5"]
["","","Hагрев","Выс.","м³/мин","15.0","15.0","18.0","18.0","29.0","34.0","34.0"]
["","","Нагрев","Средн.","м³/мин","12.5","12.5","15.0","15.0","24.5","29.0","29.0"]
["","","Hагрев","Низк.","м³/мин","10.5","10.5","12.5","12.5","20.0","23.5","23.5"]
["","Внешнее статическое давление","","Ном.","Па","30","30","30","30","40","50","50"]
["Уровень звуковой мощности","Охлаждение","","","дБA","60.0","60.0","56.0","56.0","58.0","62.0","62.0"]
["Уровень звукового давления","Охлаждение","","Выс.","дБA","35.0","35.0","30.0","30.0","34.0","37.0","37.0"]
["","","","Средн.","дБA","32.0","32.0","28.0","28.0","32.0","35.0","35.0"]
["","","","Низк.","дБA","29.0","29.0","25.0","25.0","30.0","32.0","32.0"]
["","Hагрев","","Выс.","дБA","37.0","37.0","31.0","31.0","36.0","38.0","38.0"]
["","Нагрев","","Средн.","дБA","34.0","34.0","28.0","28.0","33.0","35.0","35.0"]
["","Hагрев","","Низк.","дБA","29.0","29.0","25.0","25.0","30.0","32.0","32.0"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Газ","","НД","мм","9.52","12.70","12.70","15.90","15.90","15.90","15.90"]
["","Дренаж","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Высота подъема дренажа","мм","","","","625","625","625","625","625","625","625"]
["Системы управления","Инфракрасный пульт ДУ","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["","Проводной пульт дистанционного управления","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8","8","8","8"]
["","Operation manual","","","","1","1","1","1","1","1","1"]
["","Clamps","","","","4","4","4","4","4","4","4"]
["","Drain hose","","","","1","1","1","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2","2","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","1","1","1","1"]
["","Screws","","","","40","40","40","40","40","40","40"]
["","Sealing pads","","","","5","5","5","5","5","5","5"]
["Электропитание","Фаза","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Частота","","","Гц","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Напряжение","","","В","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]