{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZQ-C"]
[]
[]
[]
[]
["","","","","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQ200C7Y1B","FCAG60BVEB / FCAG60BVEB / FCAG60BVEB / FCAG60BVEB / RZQ250C7Y1B"]
["Холодопроизводительность","Ном.","","кВт","20.0 (1)","24.1 (1)"]
["Теплопроизводительность","Ном.","","кВт","23.0 (2)","26.4 (2)"]
["Охлаждение помещений","Производительность","Pрасч.","кВт","20.0","24.1"]
["","SEER","","","5.60","5.09"]
["","Годовое потребление энергии","","кВтч/г","2,145","2,842"]
["Отопление (Умеренный климат)","Capacity","Pрасч.","кВт","11.2","12.1"]
["","SCOP/A","","","3.51","3.59"]
["","Годовое потребление энергии","","кВтч/г","4,464","4,700"]
["Примечания","","","","(1) - Охлаждение: темп. в помещении: 27°CDB, 19°CWB; темп. наружного воздуха 35°CDB; эквивалентная длина трубопроводов: 7,5м; перепад уровня: 0 м","(1) - Охлаждение: темп. в помещении: 27°CDB, 19°CWB; темп. наружного воздуха 35°CDB; эквивалентная длина трубопроводов: 7,5м; перепад уровня: 0 м"]
["","","","","(2) - Нагрев: темп. в помещении: 20°CDB; темп. наружного воздуха 7°CDB, 6°CWB; эквивалентная длина труб с хладагентом: 7,5м; перепад уровня: 0 м","(2) - Нагрев: темп. в помещении: 20°CDB; темп. наружного воздуха 7°CDB, 6°CWB; эквивалентная длина труб с хладагентом: 7,5м; перепад уровня: 0 м"]
["","","","","(3) - Это значение не учитывает снижение производительности при размораживании.","(3) - Это значение не учитывает снижение производительности при размораживании."]