{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Уровень звукового давления","Hагрев","","Выс.","дБA","35.0","35.0"]
["","","","Низк.","дБA","29.0","29.0"]
["","Охлаждение","","Низк.","дБA","28.0","28.0"]
["","","","Выс.","дБA","35.0","35.0"]
["Стандартные аксессуары","Руководство по установке и эксплуатации","","","","1","1"]
["","Воздушный фильтр на всасывании","","","","1","1"]
["Системы управления","Проводной пульт дистанционного управления","","","","BRC1D52, BRC1E52A/B"]
["Piping connections","Жидкость","","НД","mm","6.35"]
["","Газ","","НД","mm","9.52"]
["","Drain","","","","27.2"]
["Уровень звуковой мощности","Охлаждение","","","дБA","55","55"]
["","Отопление","","","дБA","55","55"]
["Размеры","Блок","","Ширина","mm","652","652"]
["","","","Глубина","mm","502","502"]
["","","","Высота","mm","230","230"]
["Корпус","Материал","","","","Оцинкованная низкоуглеродистая сталь","Оцинкованная низкоуглеродистая сталь"]
["Масса","Блок","","","кг","17.0","17.0"]
["Вентилятор","Расход воздуха","Hагрев","Выс.","м³/мин","","6.95"]
["","","","Низк.","м³/мин","","5.20"]
["","","Охлаждение","Низк.","м³/мин","","5.20"]
["","","","Выс.","м³/мин","","6.50"]
["Power supply","Фаза","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Наименование","","","","V1","V1"]
["","Напряжение","","","V","230","230 +/-10%"]
["Примечания","","","","","(1) - Величина уровня звука измеряется в безэховом помещении.","(1) - Величина уровня звука измеряется в безэховом помещении."]
["","","","","","(2) - Это относительная величина, которая зависит от указанного расстояния и акустики среды. Более подробно см. чертежи с описанием уровней шума.","(2) - Это относительная величина, которая зависит от указанного расстояния и акустики среды. Более подробно см. чертежи с описанием уровней шума."]
["","","","","","(3) - Уровень звуковой мощности является абсолютной величиной, указывающей мощность, производимую источником звука.","(3) - Уровень звуковой мощности является абсолютной величиной, указывающей мощность, производимую источником звука."]
["Piping connections","Жидкость","","НД","mm","","6.35"]
["","Газ","","НД","mm","","9.52"]
["","Drain","","","","","27.2"]