{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / 3MXM-N"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B / FDXM25F3V1B / 3MXM52N2V1B"]
["Холодопроизводительность","Ном.","","кВт","5.0"]
["Охлаждение помещений","SEER","","","6.36"]
["","Годовое потребление энергии","","кВтч/г","276"]
["","Производительность","Pрасч.","кВт","5.00"]
["","Класс энергоэффективности","","","A++"]
["Отопление (Умеренный климат)","Capacity","Pрасч.","кВт","4.80"]
["","SCOP/A","","","3.83"]
["","Класс энергоэффективности","","","A"]
["","Годовое потребление энергии","","кВтч/г","1,754"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","606"]
["","EER","","","4.12"]
["","COP","","","3.69"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A"]
["","","Нагрев","","A"]
["Теплопроизводительность","Ном.","","кВт","6.80"]
["Примечания","","","","(1) - Электрические параметры см. в отдельных чертежах"]