{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RXM-A"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B9 / RXM50A5V1B","FDXM60F3V1B9 / RXM60A5V1B"]
["Холодопроизводительность","Мин.","","kW","1.70","1.7"]
["","Ном.","","kW","5.00","6"]
["","Макс.","","kW","5.30","6.5"]
["Теплопроизводительность","Мин.","","kW","1.70","1.7"]
["","Ном.","","kW","5.80","7"]
["","Макс.","","kW","6.00","7.1"]
["Номинальная эффективность","EER","","","3.06","2.93"]
["","COP","","","3.10","3.21"]
["","Годовое потребление энергии","","кВтч","817","1024"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","B","C"]
["","","Нагрев","","D","C"]
["Охлаждение помещений","Класс энергоэффективности","","","A+","A"]
["","Производительность","Pрасч.","kW","5.00","6"]
["","SEER","","","5.77","5.56"]
["","Годовое потребление энергии","","кВтч/г","303","378"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A","A"]
["","Производительность","Pрасч.","kW","4.00","4.6"]
["","SCOP/A","","","3.93","3.8"]
["","Pdh Теплопроизводительность при -10°","","kW","3.54","3.94"]
["","Годовое потребление энергии","","кВтч/г","1424","1693"]
["Примечания","","","","","(1) - Номинальные значения холодопроизводительности основаны на: темп. внутри помещения: 27°C с.т., 19°С вл.т., температура наружного воздуха: 35°C c.т., эквивалентная длина трубы с хладагентом: 5 м, перепад высот: 0 м."]
["","","","","","(2) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м."]
["","","","","","(3) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","(4) - Электрические параметры см. в отдельных чертежах"]