{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":9,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB / FDXS50F2VEB / RZQSG100L8Y1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQSG100L8Y1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQSG125L8Y1B","FDXS50F2VEB / FDXS50F2VEB / FDXS50F2VEB / RZQSG125L8Y1B","FDXS60F2VEB / FDXS60F2VEB / RZQSG125L8Y1B"]
["Охлаждение помещений","SEER","","","5.10","4.8","4.8","4.80","4.8"]
["","Годовое потребление энергии","","кВтч/г","652","693","875","875","875"]
["","Производительность","Pрасч.","kW","9.50","9.5","12","12.00","12"]
["","Класс энергоэффективности","","","A","B","B","B","B"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","kW","7.60","7.1","7.6","7.60","7.6"]
["","SCOP/A","","","3.80","3.8","3.8","3.80","3.8"]
["","Класс энергоэффективности","","","A","A","A","A","A"]
["","Годовое потребление энергии","","кВтч/г","2,800","2,616","2,800","2,800","2,800"]
["Примечания","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]