{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RZAG-A"]
[]
[]
[]
[]
["","","","","FFA35A2VEB9 / RZAG35A2V1B","FFA50A2VEB9 / RZAG35A2V1B","FFA50A2VEB9 / RZAG50A2V1B","FFA60A2VEB9 / RZAG60A2V1B","FFA60A2VEB9 / RZAG50A2V1B"]
["Холодопроизводительность","Мин.","","кВт","1.6","1.6","1.7","1.7","1.7"]
["","Макс.","","кВт","4.5","4.5","6.0","6.5","6.0"]
["","Ном.","","кВт","3.5","3.5","5.0","6.0","5.0"]
["Охлаждение помещений","SEER","","","6.40","6.81","6.30","5.80","6.43"]
["","Годовое потребление энергии","","кВтч/г","191","180","278","362","272"]
["","Производительность","Pрасч.","кВт","3.50","3.50","5.00","6.00","5.00"]
["","Класс энергоэффективности","","","A++","A++","A++","A+","A++"]
["Отопление (Умеренный климат)","Capacity","Pрасч.","кВт","4.20","4.20","4.30","4.50","4.30"]
["","SCOP/A","","","3.80","4.04","4.01","4.04","4.08"]
["","Класс энергоэффективности","","","A","A+","A+","A+","A+"]
["","Годовое потребление энергии","","кВтч/г","1,546","1,455","1,501","1,558","1,474"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","438","412","735","929","691"]
["","EER","","","4.00","4.25","3.40","3.23","3.62"]
["","COP","","","3.71","3.94","3.10","2.90","3.15"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A","A","A","A"]
["","","Нагрев","","A","A","D","D","D"]
["Теплопроизводительность","Ном.","","кВт","4.00","4.00","5.80","7.00","5.80"]
["","Мин.","","кВт","1.40","1.40","1.50","1.60","1.50"]
["","Макс.","","кВт","5.00","5.00","6.00","7.50","6.00"]