{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":7,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RXM-A"]
[]
[]
[]
[]
["","","","","FHA50AVEB98 / RXM50A5V1B","FHA50AVEB99 / RXM50A5V1B","FHA60AVEB98 / RXM60A5V1B"]
["Холодопроизводительность","Ном.","","кВт","5.00","5.00","5.7"]
["Теплопроизводительность","Ном.","","кВт","6.00","6.00","7.2"]
["Номинальная эффективность","EER","","","3.21","3.21","3.29"]
["","COP","","","3.35","3.35","3.32"]
["","Годовое потребление энергии","","кВтч","779","779","866"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A","A"]
["","","Нагрев","","C","C","C"]
["Охлаждение помещений","Класс энергоэффективности","","","A+","A+","A+"]
["","Производительность","Pрасч.","кВт","5.00","5.00","5.7"]
["","SEER","","","5.92","5.92","6.08"]
["","Годовое потребление энергии","","кВтч/г","295","295","328"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A","A","A"]
["","Производительность","Pрасч.","кВт","4.35","4.35","4.71"]
["","SCOP/A","","","3.86","3.86","3.87"]
["","Pdh Теплопроизводительность при -10°","","кВт","3.85","3.85","4.08"]
["","Годовое потребление энергии","","кВтч/г","1577","1577","1704"]
["Примечания","","","","","","(1) - Номинальные значения холодопроизводительности основаны на: темп. внутри помещения: 27°C с.т., 19°С вл.т., температура наружного воздуха: 35°C c.т., эквивалентная длина трубы с хладагентом: 5 м, перепад высот: 0 м."]
["","","","","","","(2) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м."]
["","","","","","","(3) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","","(4) - Электрические параметры см. в отдельных чертежах"]