{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZASG-MY1"]
[]
[]
[]
[]
["","","","","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZASG100M7Y1B","FHA50AVEB / FHA50AVEB / RZASG100M7Y1B"]
["Outdoor unit","","","","RZASG100M7Y1B","RZASG100M7Y1B"]
["Холодопроизводительность","Ном.","","кВт","9.50","9.50"]
["Теплопроизводительность","Ном.","","кВт","10.8","10.8"]
["Охлаждение помещений","Класс энергоэффективности","","","A++","A+"]
["","Производительность","Pрасч.","кВт","9.50","9.50"]
["","SEER","","","7.26","5.79"]
["","Годовое потребление энергии","","кВтч/г","458","574"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A+","A"]
["","Производительность","Pрасч.","кВт","6.00","6.00"]
["","SCOP/A","","","4.02","3.92"]
["","Годовое потребление энергии","","кВтч/г","2090","2143"]
["Примечания","","","","(1) - Номинальные значения холодопроизводительности основаны на: темп. внутри помещения: 27°C с.т., 19°С вл.т., температура наружного воздуха: 35°C c.т., эквивалентная длина трубы с хладагентом: 5 м, перепад высот: 0 м.","(1) - Номинальные значения холодопроизводительности основаны на: темп. внутри помещения: 27°C с.т., 19°С вл.т., температура наружного воздуха: 35°C c.т., эквивалентная длина трубы с хладагентом: 5 м, перепад высот: 0 м."]
["","","","","(2) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м.","(2) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м."]