{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RXL-K"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB / RXL35K2V1B","FHQ50CAVEB / RXL50K2V1B"]
["Холодопроизводительность","Мин.","","kW","1.4","1.7"]
["","Макс.","","kW","4.0","5.8"]
["","Ном.","","kW","3.40","5.00"]
["Номинальная эффективность","Annual energy consumption","","кВтч","475","785"]
["","EER","","","3.58","3.18"]
["","COP","","","3.96","3.35"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","B"]
["","","Нагрев","","A","C"]
["Теплопроизводительность","Ном.","","kW","4.00","6.00"]
["","Мин.","","kW","1.3","1.6"]
["","Макс.","","kW","5.1","6.8"]
["Примечания","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]