{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Уровень звукового давления","Hагрев","Выс.","дБ(A)","46"]
["","","Тихая работа","дБ(A)","30"]
["","","Низк.","дБ(A)","33"]
["","Охлаждение","Тихая работа","дБ(A)","29"]
["","","Низк.","дБ(A)","32"]
["","","Выс.","дБ(A)","38"]
["","","Ном.","дБ(A)","36"]
["","Охлаждение","Ном.","дБ(A)","35"]
["Стандартные аксессуары","Инструкции по установке","","","1"]
["","Руководство по эксплуатации","","","1"]
["","Пульт дистанционного управления","","","1"]
["","Сухие батареи AAA","","","2"]
["","Держатель пульта дистанционного управления","","","1"]
["","Монтажная пластина","","","1"]
["","Теплоизолированная трубка (трубка с хладагентом)","","","8"]
["","Фильтр для очистки воздуха","","","1"]
["","Фотокаталитический дезодорирующий фильтр","","","1"]
["","Боковая крышка","","","2"]
["","Бандажная лента","","","4"]
["Системы управления","Infrared remote control","","","ARC433B67"]
["Подсоединение труб","Жидкость","НД","мм","6.35"]
["","Газ","НД","мм","9.5"]
["","Дренаж","","","18"]
["Sound power level","Охлаждение","","дБ(A)","53"]
["","Отопление","","дБ(A)","59"]
["Размеры","Блок","Ширина","мм","1,050"]
["","","Глубина","мм","200"]
["","","Высота","мм","490"]
["Корпус","Цвет","","","Миндаль"]
["Масса","Блок","","kg","16"]
["Power supply","Фаза","","","1~"]
["","Частота","","Гц","50"]
["","Наименование","","","VM"]
["","Напряжение","","В","220-240"]
["Примечания","","","","(1) - 220 В"]
["","","","","(2) - 230 В"]
["","","","","(3) - 240В"]
["","","","","(4) - При подсоединении к наружному блоку многоблочной системы, см. технические характеристики подсоединяемого наружного блока."]