{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":9,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9"]
[]
[]
[]
[]
["","","","","","FNA25A2VEB9","FNA35A2VEB9","FNA50A2VEB9","FNA60A2VEB9"]
["Уровень звукового давления","Hагрев","","Выс.","дБ(A)","33.0","33.0","36.0","36.0"]
["","","","Ном.","дБ(A)","31.0","31.0","33.0","33.0"]
["","","","Низк.","дБ(A)","28.0","28.0","30.0","30.0"]
["","Охлаждение","","Средн.","дБ(A)","31.0","31.0","33.0","33.0"]
["","","","Низк.","дБ(A)","28.0","28.0","30.0","30.0"]
["","","","Выс.","дБ(A)","33.0","33.0","36.0","36.0"]
["Control systems","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["","Infrared remote control","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Подсоединения труб","Liquid","","OD","мм","6.35","6.35","6.35","6.35"]
["","Газ","","НД","мм","9.52","9.52","12.7","12.7"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Охлаждение","","","дБ(A)","53.0","53.0","56.0","56.0"]
["Размеры","Блок","","Ширина","мм","790","790","1,190","1,190"]
["","","","Глубина","мм","200","200","200","200"]
["","","","Высота","мм","620, 720 (1)","620, 720 (1)","620, 720 (1)","620, 720 (1)"]
["Casing","Material","","","","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали"]
["","Цвет","","","","Не окрашен","Не окрашен","Не окрашен","Не окрашен"]
["Вес","Блок","","","кг","23.0","23.0","30.0","30.0"]
["Fan","Внешнее статическое давление","","Выс.","Па","48","48","49","49"]
["","","","Ном.","Па","30","30","40","40"]
["","Расход воздуха","Hагрев","Выс.","м³/мин","8.7","8.7","16.0","16.0"]
["","","","Низк.","м³/мин","7.3","7.3","13.5","13.5"]
["","","","Ном.","м³/мин","8.0","8.0","14.8","14.8"]
["","","Охлаждение","Низк.","м³/мин","7.3","7.3","13.5","13.5"]
["","","","Ном.","м³/мин","8.0","8.0","14.8","14.8"]
["","","","Выс.","м³/мин","8.7","8.7","16.0","16.0"]
["Power supply","Фаза","","","","1~","1~","1~","1~"]
["","Наименование","","","","VE","VE","VE","VE"]
["","Частота","","","Гц","50/60","50/60","50/60","50/60"]
["","Напряжение","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Примечания","","","","","(1) - С установочными подставками","(1) - С установочными подставками","(1) - С установочными подставками","(1) - С установочными подставками"]
["","","","","","(2) - Уровень звуковой мощности является абсолютной величиной, указывающей мощность, производимую источником звука.","(2) - Уровень звуковой мощности является абсолютной величиной, указывающей мощность, производимую источником звука.","(2) - Уровень звуковой мощности является абсолютной величиной, указывающей мощность, производимую источником звука.","(2) - Уровень звуковой мощности является абсолютной величиной, указывающей мощность, производимую источником звука."]