{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNQ-A"]
[]
[]
[]
[]
["","","","","FNQ25A2VEB","FNQ35A2VEB","FNQ50A2VEB","FNQ60A2VEB"]
["Уровень звукового давления","Hагрев","Выс.","дБ(A)","33","33","36","36"]
["","","Ном.","дБ(A)","31","31","33","33"]
["","","Низк.","дБ(A)","28","28","30","30"]
["","Охлаждение","Низк.","дБ(A)","28","28","30","30"]
["","","Выс.","дБ(A)","33","33","36","36"]
["","","Ном.","дБ(A)","31","31","33","33"]
["Хладагент","ПГП","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["Системы управления","Проводной пульт дистанционного управления","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Холодопроизводительность","Общая производительность","Ном.","кВт","2.6","3.4","5.0","6.0"]
["Подсоединение труб","Жидкость","НД","мм","6.35","6.35","6.35","6.35"]
["","Газ","НД","мм","9.52","9.52","12.7","12.7"]
["","Дренаж","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Уровень звуковой мощности","Охлаждение","","дБ(A)","53","53","56","56"]
["Размеры","Блок","Ширина","мм","790","790","1,190","1,190"]
["","","Глубина","мм","200","200","200","200"]
["","","Высота","мм","620, 720 (2)","620, 720 (2)","620, 720 (2)","620, 720 (2)"]
["Корпус","Материал","","","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали"]
["","Цвет","","","Не окрашен","Не окрашен","Не окрашен","Не окрашен"]
["Масса","Блок","","кг","23","23","30","30"]
["Вентилятор","Внешнее статическое давление","Выс.","Па","48","48","49","49"]
["","","Ном.","Па","30","30","40","40"]
["Теплопроизводительность","Общая производительность","Ном.","кВт","3.2","4.0","5.8","7.0"]
["Power supply","Фаза","","","1~","1~","1~","1~"]
["","Частота","","Гц","50/60","50/60","50/60","50/60"]
["","Напряжение","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Примечания","","","","(1) - Уровень звуковой мощности является абсолютной величиной, указывающей мощность, производимую источником звука.","(1) - Уровень звуковой мощности является абсолютной величиной, указывающей мощность, производимую источником звука.","(1) - Уровень звуковой мощности является абсолютной величиной, указывающей мощность, производимую источником звука.","(1) - Уровень звуковой мощности является абсолютной величиной, указывающей мощность, производимую источником звука."]
["","","","","(2) - С установочными подставками","(2) - С установочными подставками","(2) - С установочными подставками","(2) - С установочными подставками"]