{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":88,"n_cols":14,"rows_kept":88,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-A"]
[]
[]
[]
[]
["","","","","","FTXF35A5V1B","FTXF50A2V1B","FTXF60A2V1B","FTXF71A2V1B","FTXF20A2V1B (Archived)","FTXF20A5V1B (Archived)","FTXF25A2V1B (Archived)","FTXF25A5V1B (Archived)","FTXF35A2V1B (Archived)"]
["Уровень звукового давления","Hагрев","","Выс.","дБA","40","","","","39","39","40","40","40"]
["","","","Средн.","дБA","35","","","","34","34","34","34","35"]
["","","","Тихая работа","дБA","21","","","","21","21","21","21","21"]
["","","","Низк.","дБA","29","","","","28","28","28","28","29"]
["","Охлаждение","","Средн.","дБA","34","","","","33","33","33","33","34"]
["","","","Тихая работа","дБA","20","","","","20","20","20","20","20"]
["","","","Низк.","дБA","27","","","","25","25","26","26","27"]
["","","","Выс.","дБA","43","","","","39","39","40","40","43"]
["Стандартные аксессуары","Инструкции по установке","","","","1","","","","1","1","1","1","1"]
["","Руководство по эксплуатации","","","","1","","","","1","1","1","1","1"]
["","Пульт дистанционного управления","","","","1","","","","1","1","1","1","1"]
["","Сухие батареи AAA","","","","2","","","","2","2","2","2","2"]
["","Держатель пульта дистанционного управления","","","","1","","","","1","1","1","1","1"]
["","Монтажная пластина","","","","1","","","","1","1","1","1","1"]
["","Крепежные винты внутреннего блока","","","","2","","","","2","2","2","2","2"]
["Control systems","Wired remote control","","","","BRC944B2, BRC073A1","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC470A1","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","","","","6.35","6.35","6.35","6.35","6.35"]
["","Газ","","НД","мм","9.50","","","","9.50","9.50","9.50","9.50","9.50"]
["","Дренаж","","","","18","","","","18","18","18","18","18"]
["Входная мощность","Охлаждение","","Ном.","kW","0.032","","","","0.017","0.017","0.019","0.019","0.032"]
["","Hагрев","","Ном.","kW","0.032","","","","0.020","0.020","0.020","0.020","0.032"]
["Уровень звуковой мощности","Охлаждение","","","дБA","58","","","","55","55","55","55","58"]
["","Отопление","","","дБA","58","","","","55","55","55","55","58"]
["Размеры","Блок","","Ширина","мм","770","","","","770","770","770","770","770"]
["","","","Глубина","мм","225","","","","225","225","225","225","225"]
["","","","Высота","мм","286","","","","286","286","286","286","286"]
["Корпус","Colour","","","","Белый","","","","Белый","Белый","Белый","Белый","Белый"]
["Масса","Блок","","","кг","9.00","","","","9.00","9.00","9.00","9.00","9.00"]
["Вентилятор","Расход воздуха","Hагрев","Выс.","м³/мин","11.5","","","","10.3","10.3","10.3","10.3","11.5"]
["","","","Низк.","м³/мин","7.0","","","","6.5","6.5","6.7","6.7","7.0"]
["","","","Средн.","м³/мин","9.0","","","","8.4","8.4","8.6","8.6","9.0"]
["","","","Тихая работа","м³/мин","5.3","","","","5.3","5.3","5.3","5.3","5.3"]
["","","Охлаждение","Низк.","м³/мин","6.3","","","","5.9","5.9","6.1","6.1","6.3"]
["","","","Средн.","м³/мин","8.3","","","","7.9","7.9","8.1","8.1","8.3"]
["","","","Выс.","м³/мин","11.5","","","","9.8","9.8","10.1","10.1","11.5"]
["","","","Тихая работа","м³/мин","4.5","","","","4.4","4.4","4.4","4.4","4.5"]
["Power supply","Фаза","","","","1~","","","","1~","1~","1~","1~","1~"]
["","Частота","","","Гц","50","","","","50","50","50","50","50"]
["","Напряжение","","","V","220-240","","","","220-240","220-240","220-240","220-240","220-240"]
["Входная мощность","Охлаждение","","Ном.","kW","","0.029","0.032","0.032"]
["","Hагрев","","Ном.","kW","","0.032","0.035","0.035"]
["Корпус","Цвет","","","","","Белый","Белый","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","","295","295","295"]
["","","","Ширина","мм","","990","990","990"]
["","","","Глубина","мм","","263","263","263"]
["Масса","Блок","","","кг","","13.5","13.5","13.5"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","","16.8","17.3","17.3"]
["","","","Средн.","м³/мин","","14.4","14.8","14.8"]
["","","","Низк.","м³/мин","","11.9","12.2","12.2"]
["","","","Тихая работа","м³/мин","","10.5","10.7","10.7"]
["","","Hагрев","Выс.","м³/мин","","17.3","17.9","17.9"]
["","","Нагрев","Средн.","м³/мин","","14.8","15.8","15.8"]
["","","Hагрев","Низк.","м³/мин","","12.2","12.8","12.8"]
["","","","Тихая работа","м³/мин","","10.7","11.3","11.3"]
["Уровень звуковой мощности","Охлаждение","","","дБA","","59","60","62"]
["","Отопление","","","дБA","","61","62","62"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","","43","45","46"]
["","","","Средн.","дБA","","39","41","42"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","","34","36","37"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБA","","31","33","34"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","","42","44","45"]
["","Нагрев","","Средн.","дБA","","38","40","41"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","","33","35","36"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБA","","30","32","33"]
["Подсоединение труб","Жидкость","","НД","мм","","6.35","6.35","6.35"]
["","Газ","","НД","мм","","12.7","12.7","12.7"]
["","Дренаж","","","","","18","18","18"]
["Системы управления","Инфракрасный пульт ДУ","","","","","ARC470A1","ARC470A1","ARC470A1"]
["","Проводной пульт дистанционного управления","","","","","BRC073A1","BRC073A1","BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","2","2"]
["","Operation manual","","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","2","2"]
["","Indoor unit fixing screws","","","","","2","2","2"]
["","Infrared remote control","","","","","1","1","1"]
["","Mounting plate","","","","","1","1","1"]
["","Remote control holder","","","","","1","1","1"]
["Электропитание","Наименование","","","","","V1","V1","V1"]
["","Фаза","","","","","1~","1~","1~"]
["","Частота","","","Гц","","50","50","50"]
["","Напряжение","","","V","","220-240","220-240","220-240"]