{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B / RXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B / RXF20B5V1B","FTXF25B5V1B / RXF25B5V1B"]
["Outdoor unit","","","","RXF20B5V1B","RXF25B5V1B"]
["Холодопроизводительность","Мин.","","кВт","1.3","1.3"]
["","Ном.","","кВт","2.00","2.50"]
["","Макс.","","кВт","2.6","3.0"]
["Теплопроизводительность","Мин.","","кВт","1.30","1.30"]
["","Ном.","","кВт","2.50","2.80"]
["","Макс.","","кВт","3.50","4.00"]
["Номинальная эффективность","EER","","","3.94","3.30"]
["","COP","","","4.19","4.01"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A"]
["","","Нагрев","","A","A"]
["Охлаждение помещений","Класс энергоэффективности","","","A++","A++"]
["","Производительность","Pрасч.","кВт","2.00","2.50"]
["","SEER","","","6.15","6.22"]
["","Годовое потребление энергии","","кВтч/г","114","141"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A+","A+"]
["","Производительность","Pрасч.","кВт","2.20","2.40"]
["","SCOP/A","","","4.10","4.06"]
["","Pdh Теплопроизводительность при -10°","","кВт","1.99","2.10"]
["","Годовое потребление энергии","","кВтч/г","751","827"]
["Диапазон энергоэффективности","","","","A+++ ~ D","A+++ ~ D"]