{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-F / 3MXF-B"]
[]
[]
[]
[]
["","","","","FTXF20F5V1B / FTXF20F5V1B / FTXF20F5V1B / 3MXF52B2V1B","FTXF20F5V1B / FTXF25F5V1B / FTXF25F5V1B / 3MXF68B2V1B"]
["Холодопроизводительность","Мин.","","кВт","1.80","2.00"]
["","Ном.","","кВт","5.20","6.80"]
["","Макс.","","кВт","7.00","7.25"]
["Теплопроизводительность","Мин.","","кВт","1.30","2.20"]
["","Ном.","","кВт","6.80","8.60"]
["","Макс.","","кВт","9.90","10.65"]
["Номинальная эффективность","EER","","","4.10","3.48"]
["","COP","","","3.93","3.82"]
["","Годовое потребление энергии","","кВтч","634","977"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A"]
["","","Нагрев","","A","A"]
["Охлаждение помещений","Класс энергоэффективности","","","A++","A++"]
["","Производительность","Pрасч.","кВт","5.20","6.80"]
["","SEER","","","7.61","6.61"]
["","Годовое потребление энергии","","кВтч/г","239","360"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A++","A++"]
["","Производительность","Pрасч.","кВт","5.00","5.30"]
["","SCOP/A","","","4.61","4.63"]
["","Pdh Теплопроизводительность при -10°","","кВт","3.74","3.95"]
["","Годовое потребление энергии","","кВтч/г","1519","1601"]
["Диапазон энергоэффективности","","","","A+++ ~ D","A+++ ~ D"]