{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":10,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM52N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM52N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM68N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM68N2V1B"]
["Холодопроизводительность","Ном.","","кВт","4.00","","4.00","5.20","4.00","6.00"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","467","","471","593","457","787"]
["","EER","","","4.28","","4.25","4.38","4.38","3.81"]
["","COP","","","4.32","","4.05","4.42","4.04","3.88"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","","A","A","A","A"]
["","","Нагрев","","A","","A","A","A","A"]
["Теплопроизводительность","Ном.","","кВт","4.60","","6.80","6.80","6.50","7.80"]
["Холодопроизводительность","Ном.","","кВт","","4.00"]
["Теплопроизводительность","Ном.","","кВт","","4.60"]
["Номинальная эффективность","EER","","","","4.15"]
["","COP","","","","3.95"]
["","Годовое потребление энергии","","кВтч","","482"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","","A"]
["","","Нагрев","","","A"]
["Охлаждение помещений","Класс энергоэффективности","","","","A++"]
["","Производительность","Pрасч.","кВт","","4.00"]
["","SEER","","","","7.62"]
["","Годовое потребление энергии","","кВтч/г","","164"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","","A+"]
["","Производительность","Pрасч.","кВт","","4.80"]
["","SCOP/A","","","","4.11"]
["","Pdh Теплопроизводительность при -10°","","кВт","","3.58"]
["","Годовое потребление энергии","","кВтч/г","","1632"]
["Примечания","","","","","(1) - Номинальные значения холодопроизводительности основаны на: темп. внутри помещения: 27°C с.т., 19°С вл.т., температура наружного воздуха: 35°C c.т., эквивалентная длина трубы с хладагентом: 5 м, перепад высот: 0 м."]
["","","","","","(2) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м."]
["","","","","","(3) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","(4) - Электрические параметры см. в отдельных чертежах"]