{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW"]
[]
[]
[]
[]
["","","","","","FTXJ20MV1BW","FTXJ25MV1BW","FTXJ35MV1BW","FTXJ50MV1BW"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.023","0.023","0.033","0.033"]
["","Hагрев","","Ном.","кВт","0.031","0.033","0.042","0.043"]
["Корпус","Цвет","","","","Белый","Белый","Белый","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","303","303","303","303"]
["","","","Ширина","мм","998","998","998","998"]
["","","","Глубина","мм","212","212","212","212"]
["Масса","Блок","","","kg","12","12","12","12"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","8.9","8.9","10.9","10.9"]
["","","","Средн.","м³/мин","6.6","6.6","7.8","8.9"]
["","","","Низк.","м³/мин","4.4","4.4","4.8","6.8"]
["","","","Тихая работа","м³/мин","2.6","2.6","2.9","3.6"]
["","","Hагрев","Выс.","м³/мин","10.2","11.0","12.4","12.6"]
["","","Нагрев","Средн.","м³/мин","8.4","8.6","9.6","10.5"]
["","","Hагрев","Низк.","м³/мин","6.3","6.3","6.9","8.1"]
["","","","Тихая работа","м³/мин","3.8","3.8","4.1","5.0"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","54","54","59","60"]
["","Отопление","","","дБ(A)","56","56","59","60"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","38","38","45","46"]
["","","","Средн.","дБ(A)","32","32","34","40"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","25","25","26","35"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБ(A)","19","19","20","25"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","40","41","45","47"]
["","Нагрев","","Средн.","дБ(A)","34","34","37","41"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","28","28","29","35"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБ(A)","19","19","20","25"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35","6.35","6.35"]
["","Газ","","НД","мм","9.50","9.50","9.50","12.70"]
["","Дренаж","","","","18","18","18","18"]
["Системы управления","Infrared remote control","","","","ARC466A9","ARC466A9","ARC466A9","ARC466A9"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1"]
["","Screw cover","","","","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","Fixing screw for remote controller holder","","","","2","2","2","2"]
["","WLAN adapter kit","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2","2"]
["","Fixing screws for mounting plate","","","","5","5","5","5"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Электропитание","Наименование","","","","V1","V1","V1","V1"]
["","Фаза","","","","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50"]
["","Напряжение","","","В","220-240","220-240","220-240","220-240"]
["Примечания","","","","","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - 220 В"]
["","","","","","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 230 В"]
["","","","","","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 240В"]