{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-N"]
[]
[]
[]
[]
["","","","","","FTXP20N5V1B","FTXP25N5V1B","FTXP35N5V1B","FTXP50N2V1B","FTXP60N2V1B","FTXP71N2V1B"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.019","0.02","0.032","0.029","0.032","0.032"]
["","Hагрев","","Ном.","кВт","0.023","0.023","0.032","0.032","0.035","0.035"]
["Корпус","Цвет","","","","Белый","Белый","Белый","Белый","Белый","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","286","286","286","295","295","295"]
["","","","Ширина","мм","770","770","770","990","990","990"]
["","","","Глубина","мм","225","225","225","263","263","263"]
["Масса","Блок","","","kg","8.5","8.5","9","13.5","13.5","13.5"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","9.5","9.7","11.5","16.3","16.8","16.8"]
["","","","Средн.","м³/мин","7.4","7.7","8.3","14","14.4","14.4"]
["","","","Низк.","м³/мин","5.6","5.8","6.3","11.5","11.8","11.8"]
["","","","Тихая работа","м³/мин","4.2","4.2","4.5","8.3","9.2","10.1"]
["","","Hагрев","Выс.","м³/мин","10.4","10.4","11.5","17.3","17.9","17.9"]
["","","Нагрев","Средн.","м³/мин","8.1","8.1","9","14.4","15.3","15.3"]
["","","Hагрев","Низк.","м³/мин","6.2","6.4","7","11.8","12.4","12.4"]
["","","","Тихая работа","м³/мин","5.2","5.2","5.3","10.4","11","11"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","55","55","58","59","60","62"]
["","Отопление","","","дБ(A)","55","55","58","61","62","62"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","39","40","43","43","45","46"]
["","","","Средн.","дБ(A)","33","33","34","39","41","42"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","25","26","27","34","36","37"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБ(A)","19","19","20","27","30","32"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","39","40","40","42","44","45"]
["","Нагрев","","Средн.","дБ(A)","34","34","35","38","40","41"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","28","28","29","33","35","36"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБ(A)","21","21","21","30","32","33"]
["Подсоединение труб","Жидкость","","НД","мм","6","6","6","6.4","6.4","6.4"]
["","Газ","","НД","мм","9.5","9.5","9.5","12.7","12.7","12.7"]
["","Дренаж","","","","18","18","18","18","18","18"]
["Системы управления","Infrared remote control","","","","","","ARC480A78","ARC480A53","ARC480A53","ARC480A53"]
["Системы управления","Проводной пульт дистанционного управления","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1","1","1"]
["","Silver particle filter","","","","1","1","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1"]
["Электропитание","Наименование","","","","","","","V1","V1","V1"]
["","Фаза","","","","1~","1~","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50","50","50"]
["","Напряжение","","","В","220-240","220-240","220-240","220-240","220-240","220-240"]
["Системы управления","Инфракрасный пульт ДУ","","","","ARC480A78","ARC480A78"]
["Стандартные аксессуары","WLAN adapter kit","","","","","","","1","1","1"]