{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Уровень звукового давления","Hагрев","","Выс.","дБ(A)","38","39","42","42","44","","46"]
["","","","Тихая работа","дБ(A)","25","25","26","30","31","","34"]
["","","","Низк.","дБ(A)","28","28","29","33","34","","37"]
["","Охлаждение","","Тихая работа","дБ(A)","22","22","23","30","31","","34"]
["","","","Низк.","дБ(A)","25","25","26","33","34","","37"]
["","","","Выс.","дБ(A)","38","38","42","42","43","","46"]
["","","","Ном.","дБ(A)","33","34","36","38","39","","42"]
["","Охлаждение","","Ном.","дБ(A)","32","32","34","38","39","","42"]
["Стандартные аксессуары","Титано-апатитовый фотокаталитический фильтр","","","","2","2","2","2","2"]
["","Руководство по эксплуатации","","","","1","1","1","1","1","","1"]
["","Инструкции по установке","","","","1","1","1","1","1","","1"]
["","Беспроводной пульт дистанционного управления","","","","1","1","1","1","1","","1"]
["","Батареи","","","","2","2","2","2","2","","2"]
["","Держатель пульта дистанционного управления","","","","1","1","1","1","1","","1"]
["","Крепежные винты внутреннего блока","","","","2","2","2","2","2","","2"]
["","Монтажная пластина","","","","1","1","1","1","1","","1"]
["Системы управления","Infrared remote control","","","","","","","","","","ARC452A3"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Газ","","НД","мм","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Дренаж","","","","18","18","18","18","18","","18"]
["Power input","Охлаждение","","Ном.","кВт","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Hагрев","","Ном.","кВт","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Sound power level","Охлаждение","","","дБ(A)","54","54","58","58","59","","63"]
["","Отопление","","","дБ(A)","54","55","58","58","60","","62"]
["Размеры","Блок","","Ширина","мм","800","800","800","800","800","","1,050"]
["","","","Глубина","мм","215","215","215","215","215","","250"]
["","","","Высота","мм","295","295","295","295","295","","290"]
["Корпус","Цвет","","","","Белый","Белый","Белый","Белый","Белый","","Белый"]
["Масса","Блок","","","kg","9","9","10","10","10","","12"]
["Power supply","Фаза","","","","1~","1~","1~","1~","1~","","1~"]
["","Частота","","","Гц","50","50","50","50","50","","50"]
["","Наименование","","","","V1","V1","V1","V1","V1","","V1"]
["","Напряжение","","","В","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Примечания","","","","","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - SL: Тихий уровень работы вентилятора в установке расхода воздуха"]
["","","","","","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 220 В"]
["","","","","","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 230 В"]
["Вентилятор","Расход воздуха","Охлаждение","Ном.","м³/мин","","","","","","16.0"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБ(A)","","","","","","41"]
["Вентилятор","Расход воздуха","Hагрев","Ном.","м³/мин","","","","","","14.9"]
["Уровень звукового давления","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБ(A)","","","","","","40"]
["Входная мощность","Охлаждение","","Ном.","кВт","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Hагрев","","Ном.","кВт","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Корпус","Цвет","","","","","","","","","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","","","","","","290"]
["","","","Ширина","мм","","","","","","1050"]
["","","","Глубина","мм","","","","","","250"]
["Масса","Блок","","","kg","","","","","","12"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","","","","","","16.0"]
["","","","Низк.","м³/мин","","","","","","11.3"]
["","","","Тихая работа","м³/мин","","","","","","10.1"]
["","","Hагрев","Выс.","м³/мин","","","","","","17.2"]
["","","","Низк.","м³/мин","","","","","","12.6"]
["","","","Тихая работа","м³/мин","","","","","","11.3"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","","","","","","60"]
["","Отопление","","","дБ(A)","","","","","","59"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","","","","","","45"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","","","","","","36"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБ(A)","","","","","","33"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","","","","","","44"]
["","","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","","","","","","35"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБ(A)","","","","","","32"]
["Подсоединение труб","Жидкость","","НД","мм","","","","","","6.35"]
["","Газ","","НД","мм","","","","","","12.7"]
["","Дренаж","","","","","","","","","18"]
["Системы управления","Инфракрасный пульт ДУ","","","","","","","","","ARC452A3"]
["Стандартные аксессуары","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["Электропитание","Наименование","","","","","","","","","V1"]
["","Фаза","","","","","","","","","1~"]
["","Частота","","","Гц","","","","","","50"]
["","Напряжение","","","В","","","","","","220-240"]
["Стандартные аксессуары","Титано-апатитовый фотокаталитический фильтр без корпуса","","","","","","","","","","2"]
["Примечания","","","","","","","","","","","(4) - 240В"]