{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":5,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-AW"]
[]
[]
[]
[]
["","","","","FTXTA30A2V1BW"]
["Уровень звукового давления","Hагрев","Выс.","дБA","41"]
["","","Средн.","дБA","31"]
["","","Тихая работа","дБA","19"]
["","","Низк.","дБA","24"]
["","Охлаждение","Medium","дБA","32"]
["","","Тихая работа","дБA","20"]
["","","Низк.","дБA","25"]
["","","Выс.","дБA","43"]
["Стандартные аксессуары","Инструкции по установке","","","1"]
["","Руководство по эксплуатации","","","1"]
["","Воздушный фильтр","","","2"]
["","Пульт дистанционного управления","","","1"]
["","Монтажная пластина пульта дистанционного управления","","","1"]
["","Пакет для винтов","","","1"]
["","Чехол для винтов","","","2"]
["","Сухие батареи AAA","","","2"]
["","Общие меры предосторожности","","","1"]
["Хладагент","ПГП","","","675.0"]
["Control systems","Wired remote control","","","BRC073A4"]
["","Infrared remote control","","","ARC466A59"]
["Подсоединение труб","Жидкость","НД","мм","6.35"]
["","Газ","НД","мм","9.50"]
["","Дренаж","","","18"]
["Входная мощность","Охлаждение","Ном.","кВт","0.023"]
["","Hагрев","Ном.","кВт","0.022"]
["Уровень звуковой мощности","Охлаждение","","дБA","60"]
["","Отопление","","дБA","60"]
["Размеры","Блок","Ширина","мм","798"]
["","","Глубина","мм","189"]
["","","Высота","мм","295"]
["Корпус","Цвет","","","Белый"]
["Масса","Блок","","кг","11.5"]
["Power supply","Фаза","","","1~"]
["","Частота","","Гц","50"]
["","Наименование","","","V1"]
["","Напряжение","","В","220-240"]