{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-BB / RXTA-C"]
[]
[]
[]
[]
["","","","","FTXTA30B2V1BB / RXTA30C2V1B"]
["Холодопроизводительность","Мин.","","kW","0.70"]
["","Ном.","","kW","3.00"]
["","Макс.","","kW","4.50"]
["Теплопроизводительность","Мин.","","kW","0.80"]
["","Ном.","","kW","3.20"]
["","Макс.","","kW","6.90"]
["Номинальная эффективность","Annual energy consumption","","kWh","357"]
["","COP","","","4.87"]
["","EER","","","4.20"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A"]
["","","Нагрев","","A"]
["Примечания","","","","(1) - Номинальные значения холодопроизводительности основаны на: темп. внутри помещения: 27°C с.т., 19°С вл.т., температура наружного воздуха: 35°C c.т., эквивалентная длина трубы с хладагентом: 5 м, перепад высот: 0 м."]
["","","","","(2) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м."]
["","","","","(3) - Электрические параметры см. в отдельных чертежах"]
["","","","","(4) - Рабочий диапазон см. в отдельных чертежах"]