{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Уровень звукового давления","Hагрев","","Выс.","дБ(A)","45.0"]
["","","","Средн.","дБ(A)","31.0"]
["","","","Тихая работа","дБ(A)","19.0"]
["","","","Низк.","дБ(A)","22.0"]
["","Охлаждение","","Средн.","дБ(A)","33.0"]
["","","","Тихая работа","дБ(A)","21.0"]
["","","","Низк.","дБ(A)","25.0"]
["","","","Выс.","дБ(A)","45.0"]
["Стандартные аксессуары","Инструкции по установке","","","","1"]
["","Руководство по эксплуатации","","","","1"]
["","Беспроводной пульт дистанционного управления","","","","1"]
["","Сухие батареи AAA","","","","2"]
["","Держатель пульта дистанционного управления","","","","1"]
["","Монтажная пластина","","","","1"]
["","Крепежные винты внутреннего блока","","","","2"]
["","Серебряный фильтр тонкой очистки","","","","1"]
["Control systems","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Подсоединение труб","Жидкость","","НД","мм","6.35"]
["","Газ","","НД","мм","9.50"]
["","Дренаж","","","","18"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.035"]
["","Hагрев","","Ном.","кВт","0.039"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","60.0"]
["","Отопление","","","дБ(A)","61.0"]
["Размеры","Блок","","Ширина","мм","778"]
["","","","Глубина","мм","272"]
["","","","Высота","мм","295"]
["Корпус","Colour","","","","Белый"]
["Масса","Блок","","","кг","10.0"]
["Вентилятор","Расход воздуха","Hагрев","Выс.","м³/мин","12.5"]
["","","","Низк.","м³/мин","4.9"]
["","","","Средн.","м³/мин","7.5"]
["","","","Тихая работа","м³/мин","4.0"]
["","","Охлаждение","Низк.","м³/мин","5.3"]
["","","","Средн.","м³/мин","7.8"]
["","","","Выс.","м³/мин","12.2"]
["","","","Тихая работа","м³/мин","4.1"]
["Power supply","Phase","","","","1~"]
["","Частота","","","Гц","50"]
["","Наименование","","","","V1"]
["","Напряжение","","","V","220-240"]
["Примечания","","","","","(1) - Охлаждение: темп. в помещении: 27°CDB, 19,0°CWB; темп. наружного воздуха 35°CDB, 24°CWB; эквивалентная длина трубопроводов: 5 м"]
["","","","","","(2) - Нагрев: темп. в помещении: 20°CDB; темп. наружного воздуха 7°CDB, 6°CWB; эквивалентная длина труб с хладагентом: 5 м"]
["","","","","","(3) - Электрические параметры см. в отдельных чертежах"]
["Входная мощность","Охлаждение","","Ном.","кВт","","0.053"]
["","Hагрев","","Ном.","кВт","","0.06"]
["Корпус","Цвет","","","","","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","","299"]
["","","","Ширина","мм","","998"]
["","","","Глубина","мм","","292"]
["Масса","Блок","","","кг","","14.5"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","","15.4"]
["","","","Средн.","м³/мин","","9.5"]
["","","","Низк.","м³/мин","","5.8"]
["","","","Тихая работа","м³/мин","","4.6"]
["","","Hагрев","Выс.","м³/мин","","17.5"]
["","","Нагрев","Средн.","м³/мин","","10.5"]
["","","Hагрев","Низк.","м³/мин","","7.1"]
["","","","Тихая работа","м³/мин","","5.9"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","","60"]
["","Отопление","","","дБ(A)","","61"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","","46"]
["","","","Средн.","дБ(A)","","32"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","","24"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБ(A)","","20"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","","46"]
["","Нагрев","","Средн.","дБ(A)","","31"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","","22"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБ(A)","","19"]
["Подсоединение труб","Жидкость","","НД","мм","","6.35"]
["","Газ","","НД","мм","","9.5"]
["","Дренаж","","","","","18"]
["Control systems","Infrared remote control","","","","","ARC466A75"]
["Системы управления","Проводной пульт дистанционного управления","","","","","BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Электропитание","Наименование","","","","","V1"]
["","Фаза","","","","","1~"]
["","Частота","","","Гц","","50"]
["","Напряжение","","","V","","220-240"]