{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Уровень звукового давления","Hагрев","","Выс.","дБA","","","","41","46","47"]
["","","","Средн.","дБA","","","","38","42","43"]
["","","","Низк.","дБA","","","","35","39","40"]
["","Охлаждение","","Средн.","дБA","","","","38","42","43"]
["","","","Низк.","дБA","","","","35","39","40"]
["","","","Выс.","дБA","","","","41","46","47"]
["Стандартные аксессуары","Руководство по эксплуатации","","","","","","","1","1","1"]
["","Инструкции по установке","","","","","","","1","1","1"]
["","Сливной шланг","","","","","","","1","1","1"]
["","Теплоизолированная труба","","","","","","","3","3","3"]
["","Хомуты","","","","","","","10","10","10"]
["","Хомут для шланга","","","","","","","1","1","1"]
["","Уплотнительный материал","","","","","","","4","4","4"]
["","Крепежная пластина шайбы","","","","","","","1","1","1"]
["","Дренажное сочленение","","","","","","","1","1","1"]
["","Нетканое полотно","","","","","","","1","1","1"]
["","Шайба","","","","","","","8","8","8"]
["","Крепежный винт для сливного шланга","","","","","","","5","5","5"]
["Системы управления","Wired remote control","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Холодопроизводительность","Total capacity","","Ном.","кВт","","","","","","12.1"]
["Подсоединения труб","Liquid","","OD","мм","","","","9.52","9.52","9.52"]
["","Газ","","НД","мм","","","","15.9","15.9","15.9"]
["","Drain","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Уровень звуковой мощности","Охлаждение","","","дБA","","","","59","64","65"]
["","Отопление","","","дБA","","","","59","64"]
["Размеры","Блок","","Ширина","мм","","","","950","950","950"]
["","","","Глубина","мм","","","","950","950","950"]
["","","","Высота","мм","","","","198","198","198"]
["Корпус","Материал","","","","","","","Полимер","Полимер","Полимер"]
["","Colour","","","","","","","Яркий белый","Яркий белый","Яркий белый"]
["Вес","Блок","","","кг","","","","25.0","26.0","26"]
["Вентилятор","Расход воздуха","Hагрев","Выс.","м³/мин","","","","23.0","31.0","32.5"]
["","","","Средн.","м³/мин","","","","19.5","25.5","26.5"]
["","","","Низк.","м³/мин","","","","16.0","20.0","20.5"]
["","","Охлаждение","Низк.","м³/мин","","","","16.0","20.0","20.5"]
["","","","Средн.","м³/мин","","","","19.5","25.5","26.5"]
["","","","Выс.","м³/мин","","","","23.0","31.0","32.5"]
["Высота подъема дренажа","мм","","","","","","","600","600","600"]
["Теплопроизводительность","Total capacity","","Ном.","кВт","","","","","","13.5"]
["Корпус","Цвет","","","","Яркий белый","Яркий белый","Яркий белый"]
["","Материал","","","","Полимер","Полимер","Полимер"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","198","198","198"]
["","","","Ширина","мм","950","950","950"]
["","","","Глубина","мм","950","950","950"]
["Масса","Блок","","","кг","25.0","26.0","26.0"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","23.0","31.0","32.5"]
["","","","Средн.","м³/мин","19.5","25.5","26.5"]
["","","","Низк.","м³/мин","16.0","20.0","20.5"]
["","","Hагрев","Выс.","м³/мин","23.0","31.0","32.5"]
["","","Нагрев","Средн.","м³/мин","19.5","25.5","26.5"]
["","","Hагрев","Низк.","м³/мин","16.0","20.0","20.5"]
["Уровень звуковой мощности","Охлаждение","","","дБA","59","64","65"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","41","46","47"]
["","","","Средн.","дБA","38","42","43"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","35","39","40"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","41","46","47"]
["","Нагрев","","Средн.","дБA","38","42","43"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","35","39","40"]
["Подсоединение труб","Жидкость","","НД","мм","9.52","9.52","9.52"]
["","Газ","","НД","мм","15.9","15.9","15.9"]
["","Дренаж","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Высота подъема дренажа","мм","","","","600","600","600"]
["Стандартные аксессуары","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Холодопроизводительность","Общая производительность","","Ном.","кВт","","","12.10"]
["Теплопроизводительность","Общая производительность","","Ном.","кВт","","","13.5"]