{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K / RXLG-M"]
[]
[]
[]
[]
["","","","","FVXG25K2V1B / RXLG25M2V1B","FVXG35K2V1B / RXLG35M2V1B"]
["Холодопроизводительность","Мин.","","кВт","1.2","1.4"]
["","Макс.","","кВт","5.1","5.6"]
["","Ном.","","кВт","2.5 (2)","3.5 (2)"]
["Подсоединения труб","Жидкость","НД","мм","6.35","6.35"]
["","Газ","НД","мм","9.5","9.5"]
["","Дренаж","OD","мм","18","18"]
["Номинальная эффективность","Годовое потребление энергии","","kWh","355","510"]
["","EER","","","3.52 (1)","3.43 (1)"]
["","COP","","","3.88 (1)","3.61 (1)"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A"]
["","","Нагрев","","A","A"]
["Теплопроизводительность","Ном.","","кВт","4.5 (2)","5.6 (2)"]
["","Мин.","","кВт","1.0 (6)","1.1 (6)"]
["","Макс.","","кВт","6.5, 3.5 (7)","7.0, 4.0 (7)"]
["Примечания","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]
["","","","","(3) - 220 В","(3) - 220 В"]
["","","","","(4) - 230 В","(4) - 230 В"]
["","","","","(5) - 240В","(5) - 240В"]
["","","","","(6) - Номинальной минимальной производительности при отоплении соответствует установка вентилятора внутреннего блока SL","(6) - Номинальной минимальной производительности при отоплении соответствует установка вентилятора внутреннего блока SL"]
["","","","","(7) - Максимальная теплопроизводительность при температуре наружного воздуха -15°C .","(7) - Максимальная теплопроизводительность при температуре наружного воздуха -15°C ."]