{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":8,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-B"]
[]
[]
[]
[]
["","","","","","FVXM25B2V1B","FVXM35B2V1B","FVXM50B2V1B"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.02","0.02","0.03"]
["","Hагрев","","Ном.","кВт","0.02","0.03","0.03"]
["Корпус","Цвет","","","","Белый","Белый","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","600","600","600"]
["","","","Ширина","мм","750","750","750"]
["","","","Глубина","мм","238","238","238"]
["Масса","Блок","","","kg","17","17","17"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","8.7","9.2","11.6"]
["","","","Средн.","м³/мин","7","7","9"]
["","","","Низк.","м³/мин","4.9","4.9","6.6"]
["","","","Тихая работа","м³/мин","4.1","4.1","5.4"]
["","","Hагрев","Выс.","м³/мин","9.2","9.8","12.8"]
["","","Нагрев","Средн.","м³/мин","7.2","7.2","10"]
["","","Hагрев","Низк.","м³/мин","5.6","5.6","8.4"]
["","","","Тихая работа","м³/мин","4.1","4.1","5.9"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","52","53","61"]
["","Отопление","","","дБ(A)","52","53","62"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","38","39","44"]
["","","","Средн.","дБ(A)","32","32","38"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","25","25","31"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБ(A)","20","20","27"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","38","39","46"]
["","Нагрев","","Средн.","дБ(A)","32","32","40"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","25","25","35"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБ(A)","19","19","29"]
["Хладагент","ПГП","","","","675","675","675"]
["Подсоединение труб","Жидкость","","НД","мм","6.4","6.4","6.4"]
["","Газ","","НД","мм","9.5","9.5","12.7"]
["","Дренаж","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Системы управления","Инфракрасный пульт ДУ","","","","ARC466A90","ARC466A90","ARC466A90"]
["","Проводной пульт дистанционного управления","","","","BRC073A1","BRC073A1","BRC073A1"]
["Стандартные аксессуары","FVXM25B2V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Электропитание","Наименование","","","","V1","V1","V1"]
["","Фаза","","","","1~","1~","1~"]
["","Частота","","","Гц","50","50","50"]
["","Напряжение","","","В","220-240","220-240","220-240"]
["Примечания","","","","","(1) - Охлаждение: темп. в помещении: 27°CDB, 19°CWB; темп. наружного воздуха 35°CDB, 24°CWB; эквивалентная длина трубопроводов: 5м","(1) - Охлаждение: темп. в помещении: 27°CDB, 19°CWB; темп. наружного воздуха 35°CDB, 24°CWB; эквивалентная длина трубопроводов: 5м","(1) - Охлаждение: темп. в помещении: 27°CDB, 19°CWB; темп. наружного воздуха 35°CDB, 24°CWB; эквивалентная длина трубопроводов: 5м"]
["","","","","","(2) - Нагрев: темп. в помещении: 20°CDB; темп. наружного воздуха 7°CDB, 6°CWB; эквивалентная длина труб с хладагентом: 5 м","(2) - Нагрев: темп. в помещении: 20°CDB; темп. наружного воздуха 7°CDB, 6°CWB; эквивалентная длина труб с хладагентом: 5 м","(2) - Нагрев: темп. в помещении: 20°CDB; темп. наружного воздуха 7°CDB, 6°CWB; эквивалентная длина труб с хладагентом: 5 м"]
["Стандартные аксессуары","FVXM35B2V1B","","","","","1"]
["","FVXM50B2V1B","","","","","","1"]