{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":9,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXG-L"]
[]
[]
[]
[]
["","","","","","RXG20L2V1B","RXG25L2V1B","RXG35L2V1B","RXG50L2V1B"]
["Уровень звукового давления","Hагрев","","Выс.","дБ(A)","","47","48"]
["","Охлаждение","","Выс.","дБ(A)","","46","48"]
["Стандартные аксессуары","Соединение (дренаж)","","","","","1","1"]
["","Инструкции по установке","","","","","1","1"]
["Хладагент","Charge","","","Экв.тонн CO2","","2.2","2.2"]
["","ПГП","","","","","2,087.5","2,087.5"]
["","Charge","","","кг","","1.05","1.05"]
["","Тип","","","","","R-410A","R-410A"]
["Мотор вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","","780","780"]
["","","Hагрев","Самый низкий","об/мин","","740","740"]
["Подсоединения труб","Перепад уровней","IU - OU","Макс.","м","","15","15"]
["","Дополнительная заправка хладагента","","","кг/м","","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)"]
["Compressor","Type","","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Размеры","Блок","","Ширина","мм","","765","765"]
["","","","Глубина","мм","","285","285"]
["","","","Высота","мм","","550","550"]
["Масса","Блок","","","кг","","35","35"]
["Вентилятор","Расход воздуха","Hагрев","Сверхнизкий","куб. фт/мин","","932","932"]
["","","Охлаждение","Сверхнизкий","куб. фт/мин","","1,094","1,094"]
["Power supply","Фаза","","","","","1~","1~"]
["","Частота","","","Гц","","50","50"]
["","Напряжение","","","V","","220-240","220-240"]
["Примечания","","","","","(1) - 220 В","(1) - SL: Тихий уровень работы вентилятора в установке расхода воздуха","(1) - SL: Тихий уровень работы вентилятора в установке расхода воздуха","(1) - 220 В"]
["","","","","","(2) - 230 В","(2) - 220 В","(2) - 220 В","(2) - 230 В"]
["","","","","","(3) - 240В","(3) - 230 В","(3) - 230 В","(3) - 240В"]
["","","","","","(4) - Рабочий диапазон в сочетании с Nexura, FVXG-K, охлаждение: мин. 10°C сух.т. – макс. 46°C сух.т.; отопление: мин. -15°C вл.т. – макс. 18°C вл.т.","(4) - 240В","(4) - 240В","(4) - Рабочий диапазон в сочетании с Nexura, FVXG-K, охлаждение: мин. 10°C сух.т. – макс. 46°C сух.т.; отопление: мин. -15°C вл.т. – макс. 18°C вл.т."]
["","","","","","","(5) - Рабочий диапазон в сочетании с Nexura, FVXG-K, охлаждение: мин. 10°C сух.т. – макс. 46°C сух.т.; отопление: мин. -15°C вл.т. – макс. 18°C вл.т.","(5) - Рабочий диапазон в сочетании с Nexura, FVXG-K, охлаждение: мин. 10°C сух.т. – макс. 46°C сух.т.; отопление: мин. -15°C вл.т. – макс. 18°C вл.т."]
["","","","","","","(6) - Содержит фторированные парниковые газы","(6) - Содержит фторированные парниковые газы"]
["Вентилятор","Расход воздуха","Охлаждение","Сверхнизкий","м³/мин","31.0","","","42.6"]
["","","Нагрев","Сверхнизкий","м³/мин","26.4","","","38.3"]
["","","","Вентилятор-=-Расход воздуха-=-Охлаждение-=-Сверхнизкий-=-фт3/мин","куб. фт/мин","1094","","","1504"]
["","","Нагрев","Вентилятор-=-Расход воздуха-=-Нагрев-=-Сверхнизкий-=-фт3/мин","куб. фт/мин","932","","","1352"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","550","","","735"]
["","","","Ширина","мм","765","","","825"]
["","","","Глубина","мм","285","","","300"]
["Масса","Блок","","","кг","35","","","48"]
["Двигатель вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","780","","","670"]
["","","Нагревание","Самый низкий","об/мин","740","","","670"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","","","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-10 (5)","","","-10 (5)"]
["","","","Макс.","°C сух.т.","46","","","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-15","","","-15"]
["","","","Макс.","°CWB","18","","","18"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","46","","","48"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","47","","","48"]
["Хладагент","Тип","","","","R-410A","","","R-410A"]
["","Заправка","","","кг","1.05","","","1.6"]
["","Заправка","","","tCO2Eq","2.2","","","3.3"]
["","ПГП","","","","2087.5","","","2087.5"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","20","","","30"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 10 м)","","","0,02 (для длины труб свыше 10 м)"]
["","перепад уровня","IU - OU","Макс.","м","15","","","20"]
["Стандартные аксессуары","Installation manual","","","","1","","","1"]
["","Joint (drain)","","","","1","","","1"]
["Электропитание","Фаза","","","","1~","","","1~"]
["","Частота","","","Гц","50","","","50"]
["","Напряжение","","","V","220-240","","","220-240"]