{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":73,"n_cols":11,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Уровень звукового давления","Hагрев","","Выс.","дБ(A)","47","47","48","48"]
["","Охлаждение","","Выс.","дБ(A)","46","46","48","48"]
["Стандартные аксессуары","Сливная крышка","","","","1","1","","1"]
["","Инструкции по установке","","","","1","1","1","1"]
["","Табличка с данными о заправке хладагентом","","","","1","1","1"]
["","Этикетки о фторированных парниковых газах на нескольких языках","","","","1","1","Этикетки о фторированных парниковых газах на нескольких языках"]
["Refrigerant","Charge","","","TCO2Eq","2.1","2.1","2.5","2.7"]
["","ПГП","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","1.0","1.0","1.20","1.3"]
["","Тип","","","","R-410A","R-410A","R-410A","R-410A"]
["Двигатель вентилятора","Скорость вращения","Охлаждение","Самый низкий","об/мин","780","780","780","790"]
["","","Нагрев","Самый низкий","об/мин","740","740","740","780"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Макс.","°C сух.т.","46","46","46","46"]
["","","","Мин.","°C сух.т.","-10","-10","-10","-10"]
["","Hагрев","Темп. нар. возд.","Макс.","°CWB","18","18","18","18"]
["","","","Мин.","°CWB","-15","-15","-15","-15"]
["Подсоединение труб","Перепад уровней","IU - OU","Макс.","м","","","15"]
["","Дополнительная заправка хладагента","","","кг/м","","","0,020 (для длины труб свыше 10 м)"]
["Размеры","Блок","","Ширина","мм","765","765","765","765"]
["","","","Глубина","мм","285","285","285","285"]
["","","","Высота","мм","550","550","550","550"]
["Компрессор","Type","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Масса","Блок","","","kg","34","34","34","39"]
["Вентилятор","Расход воздуха","Hагрев","Сверхнизкий","куб. фт/мин","904","904","904","960"]
["","","","Сверхнизкий","м³/мин","25.6","25.6","25.6","27.2"]
["","","Охлаждение","Сверхнизкий","м³/мин","30.1","30.1","30.1","30.6"]
["","","","Сверхнизкий","куб. фт/мин","1,063","1,063","1,063","1,080"]
["Power supply","Фаза","","","","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240","220-240"]
["Примечания","","","","","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - 220 В"]
["","","","","","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 230 В"]
["","","","","","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 240В"]
["","","","","","(4) - Содержит фторированные парниковые газы","(4) - Содержит фторированные парниковые газы","(4) - Содержит фторированные парниковые газы","(4) - Содержит фторированные парниковые газы"]
["Стандартные аксессуары","Сливная пробка","","","","","","1"]
["Вентилятор","Расход воздуха","Охлаждение","Сверхнизкий","м³/мин","","","","","48.9","45.0"]
["","","Нагрев","Сверхнизкий","м³/мин","","","","","43.1","46.3"]
["","","","Вентилятор-=-Расход воздуха-=-Охлаждение-=-Сверхнизкий-=-фт3/мин","куб. фт/мин","","","","","1727","1589"]
["","","Нагрев","Вентилятор-=-Расход воздуха-=-Нагрев-=-Сверхнизкий-=-фт3/мин","куб. фт/мин","","","","","1522","1635"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","","","","","735","735"]
["","","","Ширина","мм","","","","","825","825"]
["","","","Глубина","мм","","","","","300","300"]
["Масса","Блок","","","kg","","","","","47","48"]
["Двигатель вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","","","","","670"]
["","","Нагревание","Самый низкий","об/мин","","","","","670"]
["Компрессор","Тип","","","","","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","","","","","-10","-10"]
["","","","Макс.","°C сух.т.","","","","","46","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","","","","","-15","-15"]
["","","","Макс.","°CWB","","","","","18","18"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","","","","","48","49"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","","","","","44","46"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","","","","","48","49"]
["","","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","","","","","45","46"]
["Хладагент","Тип","","","","","","","","R-410A","R-410A"]
["","Заправка","","","kg","","","","","1.7","1.5"]
["","Заправка","","","tCO2Eq","","","","","3.5","3.1"]
["","ПГП","","","","","","","","2087.5","2087.5"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","","","","","30","30"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","","","","","0,020 (для длины труб свыше 10 м)","0,020 (для длины труб свыше 10 м)"]
["","перепад уровня","IU - OU","Макс.","м","","","","","20.0","20"]
["Стандартные аксессуары","Installation manual","","","","","","","","1","1"]
["","Drain plug","","","","","","","","1","1"]
["Электропитание","Фаза","","","","","","","","1~","1~"]
["","Частота","","","Гц","","","","","50","50"]
["","Напряжение","","","V","","","","","220-230-240","220-230-240"]
["Примечания","","","","","","","","","","(1) - 230 В"]