{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":74,"n_cols":9,"rows_kept":74,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-MV1"]
[]
[]
[]
[]
["","","","","","RZAG71M7V1B","RZAG100M7V1B","RZAG125M7V1B","RZAG140M7V1B"]
["Уровень звукового давления","Hагрев","","Ном.","дБ(A)","","","","52"]
["","Охлаждение","","Ном.","дБ(A)","","","","51"]
["Стандартные аксессуары","Хомуты","","","","","","","2"]
["","Инструкции по установке","","","","","","","1"]
["","Ярлык хладагента для нормы по F-газам","","","","","","","1"]
["","Общие меры предосторожности","","","","","","","1"]
["","Класс энергоэффективности LOT10","","","","","","","1"]
["Хладагент","Charge","","","TCO2Eq","","","","2.53"]
["","GWP","","","","","","","675"]
["","Заправка","","","кг","","","","3.75"]
["","Type","","","","","","","R-32"]
["Подсоединения труб","Liquid","","OD","мм","","","","9.52"]
["","Длина трубы","Макс.","НБ - ВБ","м","","","","85"]
["","","Система","Без заправки","м","","","","40"]
["","","","Равносильно","м","","","","100"]
["","Газ","","НД","мм","","","","15.9"]
["","Перепад уровней","IU - IU","Макс.","м","","","","0.5"]
["","","IU - OU","Макс.","м","","","","30.0"]
["","Дополнительная заправка хладагента","","","кг/м","","","","См. инструкции по установке"]
["Sound power level","Охлаждение","","","дБ(A)","","","","70"]
["","Отопление","","","дБ(A)","","","","70 (1)"]
["Компрессор","Тип","","","","","","","Герметичный компрессор ротационного типа"]
["Размеры","Блок","","Ширина","мм","","","","940"]
["","","","Глубина","мм","","","","320"]
["","","","Высота","мм","","","","1,430"]
["Вес","Блок","","","кг","","","","92"]
["Power supply","Фаза","","","","","","","1~"]
["","Частота","","","Гц","","","","50"]
["","Напряжение","","","V","","","","220-240"]
["Примечания","","","","","","","","(1) - Согласно ENER Lot 21"]
["","","","","","","","","(2) - Европейский/международный технический стандарт, задающий пределы гармонического тока, производимого оборудованием, подсоединенным к общедоступной сети низкого напряжения с потребляемым током больше 16A и ≤ 75A одной фазы."]
["","","","","","","","","(3) - Ssc: мощность короткого замыкания"]
["","","","","","","","","(4) - Европейский/международный технический стандарт, устанавливающий пределы гармонических токов, создаваемых оборудованием, подключенным к общедоступной сети низкого напряжения с потребляемым током ≤ 16 A на фазу"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","990","1430","1430"]
["","","","Ширина","мм","940","940","940"]
["","","","Глубина","мм","320","320","320"]
["Масса","Блок","","","кг","70","92","92"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°CDB","-20","-20","-20"]
["","","","Макс.","°CDB","52","52","52"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-20","-20","-20"]
["","","","Макс.","°CWB","18.0","18.0","18.0"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","64","66","69"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБ(A)","46","47","50"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБ(A)","49","51","52"]
["Хладагент","Тип","","","","R-32","R-32","R-32"]
["","Заправка","","","кг","2.95","3.75","3.75"]
["","ПГП","","","","675","675","675"]
["","Заправка","","","tCO2Eq","1.99","2.53","2.53"]
["Подсоединение труб","Жидкость","","НД","мм","9.52","9.52","9.52"]
["","Газ","","НД","мм","15.9","15.9","15.9"]
["","Длина трубы","Макс.","НБ - ВБ","м","55","85","85"]
["","","Система","Равносильно","м","75","100","100"]
["","","","Без заправки","м","40","40","40"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","См. инструкции по установке","См. инструкции по установке","См. инструкции по установке"]
["","перепад уровня","IU - OU","Макс.","м","30.0","30.0","30.0"]
["","","IU - IU","Макс.","м","0.5","0.5","0.5"]
["Стандартные аксессуары","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Электропитание","Фаза","","","","1~","1~","1~"]
["","Частота","","","Гц","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240"]
["Ток — 50 Гц","Макс. ток предохранителя (MFA)","","","A","20","32","32"]
["Уровень звуковой мощности","Отопление","","","дБ(A)","","","69 (1)"]
["Примечания","","","","","","","(1) - Согласно ENER Lot 21"]