{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":9,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZASG-MV1"]
[]
[]
[]
[]
["","","","","","RZASG71M2V1B","RZASG100M7V1B","RZASG125M7V1B","RZASG140M7V1B"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","770","990","990","990"]
["","","","Ширина","мм","900","940","940","940"]
["","","","Глубина","мм","320","320","320","320"]
["Масса","Блок","","","кг","60","70","70","78"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°CDB","-15","-15","-15","-15"]
["","","","Макс.","°CDB","46","46","46","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-15","-15","-15","-15"]
["","","","Макс.","°CWB","15.5","15.5","15.5","15.5"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","65","70","71","73"]
["","Отопление","","","дБ(A)","","","71 (1)","73 (1)"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБ(A)","46","53","53","54"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБ(A)","47","57","57","57"]
["Хладагент","Тип","","","","R-32","R-32","R-32","R-32"]
["","Заправка","","","кг","2.45","2.60","2.60","2.90"]
["","ПГП","","","","675","675","675","675"]
["","Заправка","","","tCO2Eq","1.65","1.76","1.76","1.96"]
["Подсоединение труб","Жидкость","","НД","мм","9.52","9.52","9.52","9.52"]
["","Газ","","НД","мм","15.9","15.9","15.9","15.9"]
["","Длина трубы","Макс.","НБ - ВБ","м","50","50","50","50"]
["","","Система","Равносильно","м","70","70","70","70"]
["","","","Без заправки","м","30","30","30","30"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","См. инструкции по установке","См. инструкции по установке","См. инструкции по установке","См. инструкции по установке"]
["","перепад уровня","IU - OU","Макс.","м","30.0","30.0","30.0","30.0"]
["","","IU - IU","Макс.","м","0.5","0.5","0.5","0.5"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1","1"]
["","Peel off F-gas label","","","","1"]
["","Tie-wraps","","","","2","2","2","2"]
["Электропитание","Фаза","","","","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240","220-240"]
["Ток — 50 Гц","Макс. ток предохранителя (MFA)","","","A","20","25","32","32"]
["Примечания","","","","","","","(1) - Согласно ENER Lot 21","(1) - Согласно ENER Lot 21"]