{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXM-A8"]
[]
[]
[]
[]
["","","","","","4MXM68A2V1B8","4MXM80A2V1B8"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","734","734"]
["","","","Ширина","мм","974","974"]
["","","","Глубина","мм","408","408"]
["Масса","Блок","","","кг","63","67"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°CDB","-10","-10"]
["","","","Макс.","°CDB","50","50"]
["Уровень звукового давления","Охлаждение","","Ном.","дБA","48","48"]
["","Hагрев","","Ном.","дБA","49","49"]
["Хладагент","Тип","","","","R-32","R-32"]
["","Заправка","","","кг","2.00","2.40"]
["","Хладагент-=-Заправка-=-Экв. т CO2","","","Экв. т CO2","1.35","1.62"]
["","ПГП","","","","675","675"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","25 (1)","25 (1)"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","002 (для длины труб свыше 30 м)","002 (для длины труб свыше 30 м)"]
["","перепад уровня","IU - OU","Макс.","м","15","15"]
["","","IU - IU","Макс.","м","7.5","7.5"]
["Подсоединение труб","Общая длина трубопроводов","Система","Фактическая","м","60","70"]
["Стандартные аксессуары","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Диапазон энергоэффективности","","","","","A+++ ~ D","A+++ ~ D"]
["Электропитание","Фаза","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Электропитание-=-Напряжение-=-В","","","В","220-240","220-240"]
["Примечания","","","","","(1) - Для одного помещения","(1) - Для одного помещения"]
["","","","","","(2) - Для комбинации с CVXM-A, FVXM-A — максимальная длина трубопровода 30 м.","(2) - Для комбинации с CVXM-A, FVXM-A — максимальная длина трубопровода 30 м."]
["","","","","","(3) - Рабочий диапазон см. в отдельных чертежах","(3) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","(4) - Электрические параметры см. в отдельных чертежах","(4) - Электрические параметры см. в отдельных чертежах"]
["","","","","","(5) - Содержит фторированные парниковые газы","(5) - Содержит фторированные парниковые газы"]