{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Стандартные аксессуары","Инструкции по установке","","","","Инструкции по установке"]
["","Руководство по эксплуатации","","","","Руководство по эксплуатации"]
["","Винт и шайба","","","","Винт и шайба"]
["","Беспроводной пульт дистанционного управления","","","","Беспроводной пульт дистанционного управления"]
["","Крышка-решетка с фиксатором","","","","Крышка-решетка с фиксатором"]
["","Батарея","","","","Батарея"]
["Подсоединение труб","Liquid","","OD","mm","9.52"]
["","Газ","","НД","mm","15.88"]
["","Дренаж","","","","19.05"]
["Входная мощность","Охлаждение","","Ном.","kW","0.128"]
["","Hагрев","","Ном.","kW","0.128"]
["Уровень звуковой мощности","Охлаждение","","","дБA","64"]
["","Отопление","","","дБA","64"]
["Размеры","Блок","","Ширина","mm","600"]
["","","","Глубина","mm","1,007"]
["","","","Высота","mm","285"]
["Корпус","Материал","","","","Оцинкованная сталь"]
["Масса","Блок","","","кг","35"]
["Вентилятор","Внешнее статическое давление","","Выс.","Па","90"]
["","","","Ном.","Па","77"]
["","","","Низк.","Па","64"]
["Power supply","Фаза","","","","1~"]
["","Частота","","","Гц","50"]
["","Наименование","","","","V1"]
["","Напряжение","","","V","220-240"]
["Входная мощность","Hагрев","","Ном.","kW","","0.109"]
["","Охлаждение","","Ном.","kW","","0.109"]
["Вентилятор","Внешнее статическое давление","","Выс.","Па","","70","150","150"]
["","","","Низк.","Па","","45","111","92"]
["Корпус","Материал","","","","","Оцинкованная сталь"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","mm","","378","378","378"]
["","","","Ширина","mm","","541","1300","1500"]
["","","","Глубина","mm","","1045","541","541"]
["Масса","Блок","","","кг","","44","50","56"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","","22.7","40.5","48.7"]
["","","","Ном.","м³/мин","","20.5","37","44"]
["","","","Низк.","м³/мин","","18.3","34.8","37.9"]
["","","Hагрев","Выс.","м³/мин","","22.7","40.5","48.7"]
["","","","Ном.","м³/мин","","20.5","37.4","43.9"]
["","","","Низк.","м³/мин","","18.3","34.8","37.9"]
["","Внешнее статическое давление","","Ном.","Па","","57","128","122"]
["Уровень звуковой мощности","Охлаждение","","","дБA","","60","72","73"]
["","Отопление","","","дБA","","60","72","73"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","","41","53","55"]
["","","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБA","","38"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","","36","50","50"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","","41","53","55"]
["","","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБA","","38"]
["","","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","","36","50","50"]
["Подсоединение труб","Жидкость","","НД","mm","","9.52","9.52","9.52"]
["","Газ","","НД","mm","","15.88","15.9","15.9"]
["","Дренаж","","","","","19.05"]
["Стандартные аксессуары","Installation manual","","","","","Installation manual"]
["","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["","Operation manual","","","","","Operation manual"]
["Электропитание","Фаза","","","","","1~"]
["","Частота","","","Гц","","50"]
["","Напряжение","","","V","","220-240"]
["Холодопроизводительность","Общая производительность","","Ном.","kW","","","12.10","13.00"]
["Теплопроизводительность","Общая производительность","","Ном.","kW","","","13.5","15.5"]
["Корпус","Цвет","","","","","","Оцинкованные металлические пластины / Неокрашенные","Оцинкованные металлические пластины / Неокрашенные"]
["Вентилятор","Расход воздуха","Охлаждение","Средн.","м³/мин","","","37","44"]
["","","Нагрев","Средн.","м³/мин","","","37.4","43.9"]
["Уровень звукового давления","Охлаждение","","Средн.","дБA","","","52","53"]
["","Нагрев","","Средн.","дБA","","","52","53"]
["Системы управления","Инфракрасный пульт ДУ","","","","","","ARCWLA","ARCWLA"]