{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","AHQ140CV1 / AZQS140B8V1B"]
["Холодопроизводительность","Ном.","","кВт","13.0 (1)"]
["Охлаждение помещений","SEER","","","5.77"]
["","Годовое потребление энергии","","кВтч/г","1,353"]
["","Производительность","Pрасч.","кВт","13.0"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","кВт","12.0"]
["","SCOP/A","","","3.99"]
["","Годовое потребление энергии","","кВтч/г","4,199"]
["Номинальная эффективность","EER","","","2.63 (3)"]
["Теплопроизводительность","Ном.","","кВт","15.5 (2)"]
["Примечания","","","","(1) - Охлаждение: темп. в помещении: 27°CDB, 19°CWB; темп. наружного воздуха 35°CDB; эквивалентная длина трубопроводов: 7,5м; перепад уровня: 0 м"]
["","","","","(2) - Нагрев: темп. в помещении: 20°CDB; темп. наружного воздуха 7°CDB, 6°CWB; эквивалентная длина труб с хладагентом: 7,5м; перепад уровня: 0 м"]
["","","","","(3) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]